(footprint "Everlight_IRM-H6xxT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Everlight IRM-H6xxT infrared remote control receiver module, https://en.everlight.com/wp-content/plugins/ItemRelationship/product_files/pdf/DMO-0000004-IRM-H6XX-TR2_Series_Datasheet_V4.pdf")
	(tags "everlight ir remote receiver")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Everlight_IRM-H6xxT"
		(at 0 3.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.15 -1.27)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -3.15 1.27)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 3.15 1.27)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 3.15 -1.27)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Everlight_IRM-H6xxT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
