(footprint "Kingbright_KPS-5130"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.kingbright.com/attachments/file/psearch/000/00/00/KPS-5130PD7C(Ver.14).pdf")
	(tags "KPS-5130 photodiode RGB sensor")
	(property "Reference" "REF**"
		(at -1.25 -2.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Kingbright_KPS-5130"
		(at 0.6 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "G"
		(at 0.5 -0.3 0)
		(layer "F.Fab")
	)
	(fp_text user "B"
		(at 0 0.7 0)
		(layer "F.Fab")
	)
	(fp_text user "R"
		(at -0.6 -0.3 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.25 -2.45 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.56 -0.85)
		(size 1.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 2.56 -0.85)
		(size 1.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.56 0.85)
		(size 1.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 2.56 0.85)
		(size 1.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Kingbright_KPS-5130.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
