(footprint "Kodenshi_LG206L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://kodenshi.co.jp/products/pdf/sensor/photointerrupter_ic/LG205L.pdf")
	(tags "Photointerrupter  infrared LED with photo IC")
	(property "Reference" "REF**"
		(at 0.2 -2.47 0)
		(layer "F.SilkS")
	)
	(property "Value" "Kodenshi_LG206L"
		(at 10.8 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.7 2.1 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.4 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.227)
	)
	(pad "2" thru_hole oval
		(at 0 2)
		(size 1.4 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 4)
		(size 1.4 1.1)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 10.3 3.27)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 10.3 0.73)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Kodenshi_LG206L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
