(footprint "Kodenshi_SG105"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "package for Kodenshi SG-105 with PCB cutout, light-direction upwards, see http://www.kodenshi.co.jp/products/pdf/sensor/photointerrupter_ref/SG-105.pdf")
	(tags "refective opto couple photo coupler")
	(property "Reference" "REF**"
		(at -2.8 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "Kodenshi_SG105"
		(at 0 4.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -1.85 -1.8)
		(end 1.85 -1.8)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.85 1.8)
		(end -1.85 -1.8)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.85 -1.8)
		(end 1.85 1.8)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.85 1.8)
		(end -1.85 1.8)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.2 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.9 -2.8)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at -0.9 2.8)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "3" smd roundrect
		(at 0.9 2.8)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "4" smd roundrect
		(at 0.9 -2.8)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Kodenshi_SG105.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
