(footprint "LaserDiode_TO38ICut-3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Laser Diode, TO-38-ICut, 3pin")
	(tags "Laser Diode TO38-ICut")
	(property "Reference" "REF**"
		(at 0.7 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "LaserDiode_TO38ICut-3"
		(at 0.7 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.7 -2.6 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0.71 0.71)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.43 0)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/LaserDiode_TO38ICut-3.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
