(footprint "Lightpipe_Dialight_515-1064F"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.dialightsignalsandcomponents.com/515-optopipe-light-pipe-trilevel-2-5mm-rnd-flat-diff-lens-press-fit/#tab-resources")
	(tags "lightpipe triple tower right angle 3mm")
	(property "Reference" "REF**"
		(at 3.2 12.8 270)
		(layer "F.SilkS")
	)
	(property "Value" "Lightpipe_Dialight_515-1064F"
		(at -4.77 10.66 270)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at -2.2 12.7 270)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.29 5.46 180)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "F&B.Cu")
	)
	(pad "" np_thru_hole circle
		(at -2.29 18.87 180)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "F&B.Cu")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Lightpipe_Dialight_515-1064F.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
