(footprint "Luna_NSL-32"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Optoisolator with LED and photoresistor")
	(tags "optoisolator")
	(property "Reference" "REF**"
		(at 5.08 -6.11 180)
		(layer "F.SilkS")
	)
	(property "Value" "Luna_NSL-32"
		(at 5.13 2.44 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.08 -1.91 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.29 1.57)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.159)
	)
	(pad "2" thru_hole oval
		(at 0 -3.81)
		(size 2.29 1.57)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 10.16 -3.17)
		(size 2.29 1.57)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 10.16 -0.64)
		(size 2.29 1.57)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Luna_NSL-32.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
