(footprint "OnSemi_CASE100CY"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "OnSemi CASE 100CY, light-direction upwards, see http://www.onsemi.com/pub/Collateral/QRE1113-D.PDF")
	(tags "refective opto couple photo coupler")
	(property "Reference" "REF**"
		(at -2.5 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_CASE100CY"
		(at 0 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.2 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.9 -2)
		(size 0.79 1.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.9 2)
		(size 0.79 1.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.9 2)
		(size 0.79 1.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.9 -2)
		(size 0.79 1.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/OnSemi_CASE100CY.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
