(footprint "Osram_SFH2201"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PhotoDiode, Clear Silicone, Osram TOPLED, 4x5.09mm, area: 2.85x2.85mm, Orientation mark at cathode, https://dammedia.osram.info/media/resource/hires/osram-dam-25688470/SFH%202201%20A01_EN.pdf")
	(tags "PhotoDiode silicone")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Osram_SFH2201"
		(at -0.08 4.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -2.265 -0.8)
		(size 0.6 1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.265 0.8)
		(size 0.6 1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.265 -0.7)
		(size 0.6 1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.265 0.7)
		(size 0.6 1)
		(layers "F.Paste")
	)
	(pad "1" smd custom
		(at -2.265 0)
		(size 0.8 3)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4 -1.5) (xy 0.03 -1.5) (xy 0.03 -1.7) (xy 0.4 -1.7) (xy 0.4 1.7) (xy 0.03 1.7) (xy 0.03 1.5)
					(xy -0.4 1.5)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 2.265 0 180)
		(size 0.8 2.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4 -1.25) (xy 0.03 -1.25) (xy 0.03 -1.4) (xy 0.4 -1.4) (xy 0.4 1.4) (xy 0.03 1.4) (xy 0.03 1.25)
					(xy -0.4 1.25)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Osram_SFH2201.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
