(footprint "Panasonic_APV-AQY_SSOP-4_4.45x2.65mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.panasonic-electric-works.com/cps/rde/xbcr/pew_eu_en/technical_information_photomos_en.pdf")
	(tags "SSOP4 APV21 AQY22")
	(property "Reference" "REF**"
		(at 0 -2.54 0)
		(layer "F.SilkS")
	)
	(property "Value" "Panasonic_APV-AQY_SSOP-4_4.45x2.65mm_P1.27mm"
		(at -0.01 2.54 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.175 -0.635)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.175 0.635)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 2.175 0.635)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 2.175 -0.635)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Panasonic_APV-AQY_SSOP-4_4.45x2.65mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
