(footprint "Sharp_GP2S700HCP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Sharp GP2S700HCP, light-direction upwards, see: https://www.sharpsde.com/fileadmin/products/Optoelectronics/Isolation%20Devices/Specs_Photointerrupter/GP2S700HCP_03Oct05_DS_D3-A02201FEN.pdf")
	(tags "refective opto couple photo coupler")
	(property "Reference" "REF**"
		(at 3.295 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "Sharp_GP2S700HCP"
		(at -3.205 0 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.65 -1.2)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1363636364)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -1.65 1.2)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1363636364)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 1.65 1.2)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1363636364)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 1.65 -1.2)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1363636364)
		(thermal_bridge_angle 45)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "keepout to avoid short circuit")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.25 -0.65) (xy -1.05 -0.65) (xy -1.05 -1.75) (xy 1.05 -1.75) (xy 1.05 -0.65) (xy 2.25 -0.65)
				(xy 2.25 0.65) (xy 1.05 0.65) (xy 1.05 1.75) (xy -1.05 1.75) (xy -1.05 0.65) (xy -2.25 0.65)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Sharp_GP2S700HCP.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
