(footprint "Sharp_GP2Y0A41SK0F"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.sharp-world.com/products/device/lineup/data/pdf/datasheet/gp2y0a41sk_e.pdf")
	(tags "Distance Sensor Sharp")
	(property "Reference" "REF**"
		(at 10.795 7.62 0)
		(layer "F.SilkS")
	)
	(property "Value" "Sharp_GP2Y0A41SK0F"
		(at 0 5.715 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "Ø->2,5 for thread M3"
		(at 19.812 -6.096 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Ø->3 for screw+nut"
		(at 19.304 -5.08 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Ø->2,5 for thread M3"
		(at -19.812 -6.096 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Ø->3 for screw+nut"
		(at -19.812 -5.08 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Emitter"
		(at -10.3 0 0)
		(layer "F.Fab")
	)
	(fp_text user "Detect"
		(at 9.4 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -18.5 0)
		(size 6.1 6.1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 18.5 0)
		(size 6.1 6.1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Sharp_GP2Y0A41SK0F.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
