(footprint "Vishay_CAST-3Pin"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "IR Receiver Vishay TSOP-xxxx, CAST package, see https://www.vishay.com/docs/82493/tsop311.pdf")
	(tags "IRReceiverVishayTSOP-xxxx CAST")
	(property "Reference" "REF**"
		(at 3.8 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_CAST-3Pin"
		(at 3.4 4.8 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.8 1.017 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.178)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 7.62 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Vishay_CAST-3Pin.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
