(footprint "Vishay_TCRT5000"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "IR Reflective Optical Sensor with Transistor Output TCRT5000 https://www.vishay.com/docs/83760/tcrt5000.pdf")
	(tags "IR Reflective Optical Sensor with Transistor Output TCRT5000 Vishay Distance Sensor")
	(property "Reference" "REF**"
		(at 2.75 -2.53 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_TCRT5000"
		(at 2.75 5.37 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" "https://www.vishay.com/docs/83760/tcrt5000.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.75 1.27 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.9 3.72)
		(size 1 1)
		(drill 1)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.75 -0.63)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.75 3.17)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.5 2.54)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.5 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/Vishay_TCRT5000.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
