(footprint "Oscillator_OCXO_Morion_MV267"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.morion.com.ru/catalog_pdf/MV267.pdf")
	(tags "OCXO")
	(property "Reference" "REF**"
		(at 0.02 -6.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_OCXO_Morion_MV267"
		(at 0.02 17.74 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Us"
		(at 20.2 38 0)
		(layer "F.SilkS")
	)
	(fp_text user "Uin"
		(at 20.3 3 0)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -20.4 38 0)
		(layer "F.SilkS")
	)
	(fp_text user "Uref"
		(at 0.02 3 0)
		(layer "F.SilkS")
	)
	(fp_text user "RF"
		(at -20.3 3 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.15 21.85 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 20.3 40.6)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -20.3 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -20.3 40.6)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 20.3 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_OCXO_Morion_MV267.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
