(footprint "Oscillator_SMD_Fordahl_DFAS2-4Pin_7.3x5.1mm_HandSoldering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mminiature Crystal Clock Oscillator TXCO Fordahl DFA S2-KS/LS/US, http://www.iqdfrequencyproducts.com/products/details/iqxo-70-11-30.pdf, hand-soldering, 7.3x5.1mm^2 package")
	(tags "SMD SMT crystal oscillator hand-soldering")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_Fordahl_DFAS2-4Pin_7.3x5.1mm_HandSoldering"
		(at 0 5.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.61 2.7)
		(size 1.54 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.61 2.7)
		(size 1.54 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.61 -2.7)
		(size 1.54 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.61 -2.7)
		(size 1.54 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_Fordahl_DFAS2-4Pin_7.3x5.1mm_HandSoldering.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
