(footprint "Oscillator_SMD_OCXO_ConnorWinfield_OH300"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.conwin.com/datasheets/cx/cx282.pdf")
	(tags "OCXO")
	(property "Reference" "REF**"
		(at -11.176 -12.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_OCXO_ConnorWinfield_OH300"
		(at 0 13 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Note1: top layer is keepout"
		(at -1 -6 0)
		(layer "Cmts.User")
	)
	(fp_text user "Note2: 2nd layer GND"
		(at 0 -4 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -11.4935 -8.89 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -11.4935 0 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -11.4935 8.89 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 11.4935 8.89 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 11.4935 3.81 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 11.4935 -3.81 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 11.4935 -8.89 270)
		(size 3.048 3.175)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_OCXO_ConnorWinfield_OH300.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
