(footprint "Oscillator_SMD_SI570_SI571_Standard"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SI570, SI571, Programmable oscillator, Standard")
	(tags "SI570 SI571 Programmable oscillator Standard")
	(property "Reference" "REF**"
		(at 0 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_SI570_SI571_Standard"
		(at -0.1 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.5 2.1)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 2.1)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.5 2.1)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.5 -2.1)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0 -2.1)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.5 -2.1)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.85 0)
		(size 1.55 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.85 0)
		(size 1.55 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SI570_SI571_Standard.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
