(footprint "Oscillator_SMD_SeikoEpson_TG2520SMN-xxx-xxxxxx-4Pin_2.5x2.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Miniature Crystal Clock Oscillator TG2520 series, https://support.epson.biz/td/api/doc_check.php?dl=app_TG2520SMN&lang=en")
	(tags "Miniature Crystal Clock Oscillator TG2520 series SMD SMT")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_SeikoEpson_TG2520SMN-xxx-xxxxxx-4Pin_2.5x2.0mm"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.7 -1.05)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.7 1.05)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.7 1.05)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.7 -1.05)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.SilkS")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -0.15 -1.3) (xy 0.15 -1.3) (xy 0.15 -0.6) (xy 1 -0.6) (xy 1 0.6) (xy 0.15 0.6) (xy 0.15 1.25)
				(xy -0.15 1.25) (xy -0.15 0.6) (xy -1 0.6) (xy -1 -0.6) (xy -0.15 -0.6)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_TG2520SMN-xxx-xxxxxx-4Pin_2.5x2.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
