(footprint "Oscillator_SMD_SiT_PQFN-4Pin_2.5x2.0mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "mems programmable oscillator https://www.sitime.com/datasheet/SiT8008 page 10, 2.5x2.0mm^2 package, generated by make_crystal.py")
	(tags "SMD SMT oscillator mems programmable")
	(property "Reference" "REF**"
		(at 0 -2.26 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_SiT_PQFN-4Pin_2.5x2.0mm"
		(at 0 2.26 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 0.75)
		(size 1.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.95 0.75)
		(size 1.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.95 -0.75)
		(size 1.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.95 -0.75)
		(size 1.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SiT_PQFN-4Pin_2.5x2.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
