(footprint "Analog_BGA-209_9.5x16mm_Layout11x19_P0.8mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Analog BGA-209 (Reference LTC DWG#05-08-1561 Rev B), 9.5x16.0mm, 209 Ball, 11x19 Layout, 0.8mm Pitch, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-bga/05081561_bga209.pdf")
	(tags "BGA 209 0.8")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Analog_BGA-209_9.5x16mm_Layout11x19_P0.8mm"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -4 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A10" smd circle
		(at 3.2 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A11" smd circle
		(at 4 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -3.2 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -2.4 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at -1.6 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at -0.8 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 0 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at 0.8 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A8" smd circle
		(at 1.6 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A9" smd circle
		(at 2.4 -7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -4 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B10" smd circle
		(at 3.2 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B11" smd circle
		(at 4 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -3.2 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -2.4 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -1.6 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at -0.8 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 0 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at 0.8 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at 1.6 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B9" smd circle
		(at 2.4 -6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -4 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C10" smd circle
		(at 3.2 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C11" smd circle
		(at 4 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -3.2 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -2.4 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at -1.6 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at -0.8 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 0 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at 0.8 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C8" smd circle
		(at 1.6 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at 2.4 -5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -4 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D10" smd circle
		(at 3.2 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D11" smd circle
		(at 4 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -3.2 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -2.4 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at -1.6 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at -0.8 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at 0 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D7" smd circle
		(at 0.8 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D8" smd circle
		(at 1.6 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D9" smd circle
		(at 2.4 -4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -4 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E10" smd circle
		(at 3.2 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E11" smd circle
		(at 4 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -3.2 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -2.4 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at -1.6 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E5" smd circle
		(at -0.8 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E6" smd circle
		(at 0 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E7" smd circle
		(at 0.8 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E8" smd circle
		(at 1.6 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E9" smd circle
		(at 2.4 -4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -4 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F10" smd circle
		(at 3.2 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F11" smd circle
		(at 4 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -3.2 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -2.4 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at -1.6 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F5" smd circle
		(at -0.8 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at 0 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F7" smd circle
		(at 0.8 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F8" smd circle
		(at 1.6 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F9" smd circle
		(at 2.4 -3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -4 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G10" smd circle
		(at 3.2 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G11" smd circle
		(at 4 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -3.2 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -2.4 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at -1.6 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G5" smd circle
		(at -0.8 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G6" smd circle
		(at 0 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G7" smd circle
		(at 0.8 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G8" smd circle
		(at 1.6 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G9" smd circle
		(at 2.4 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H1" smd circle
		(at -4 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H10" smd circle
		(at 3.2 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H11" smd circle
		(at 4 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H2" smd circle
		(at -3.2 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H3" smd circle
		(at -2.4 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H4" smd circle
		(at -1.6 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H5" smd circle
		(at -0.8 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H6" smd circle
		(at 0 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H7" smd circle
		(at 0.8 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H8" smd circle
		(at 1.6 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H9" smd circle
		(at 2.4 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J1" smd circle
		(at -4 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J10" smd circle
		(at 3.2 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J11" smd circle
		(at 4 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J2" smd circle
		(at -3.2 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J3" smd circle
		(at -2.4 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J4" smd circle
		(at -1.6 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J5" smd circle
		(at -0.8 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J6" smd circle
		(at 0 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J7" smd circle
		(at 0.8 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J8" smd circle
		(at 1.6 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J9" smd circle
		(at 2.4 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K1" smd circle
		(at -4 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K10" smd circle
		(at 3.2 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K11" smd circle
		(at 4 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K2" smd circle
		(at -3.2 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K3" smd circle
		(at -2.4 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K4" smd circle
		(at -1.6 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K5" smd circle
		(at -0.8 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K6" smd circle
		(at 0 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K7" smd circle
		(at 0.8 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K8" smd circle
		(at 1.6 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K9" smd circle
		(at 2.4 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L1" smd circle
		(at -4 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L10" smd circle
		(at 3.2 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L11" smd circle
		(at 4 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L2" smd circle
		(at -3.2 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L3" smd circle
		(at -2.4 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L4" smd circle
		(at -1.6 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L5" smd circle
		(at -0.8 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L6" smd circle
		(at 0 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L7" smd circle
		(at 0.8 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L8" smd circle
		(at 1.6 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L9" smd circle
		(at 2.4 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M1" smd circle
		(at -4 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M10" smd circle
		(at 3.2 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M11" smd circle
		(at 4 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M2" smd circle
		(at -3.2 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M3" smd circle
		(at -2.4 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M4" smd circle
		(at -1.6 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M5" smd circle
		(at -0.8 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M6" smd circle
		(at 0 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M7" smd circle
		(at 0.8 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M8" smd circle
		(at 1.6 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M9" smd circle
		(at 2.4 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N1" smd circle
		(at -4 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N10" smd circle
		(at 3.2 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N11" smd circle
		(at 4 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N2" smd circle
		(at -3.2 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N3" smd circle
		(at -2.4 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N4" smd circle
		(at -1.6 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N5" smd circle
		(at -0.8 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N6" smd circle
		(at 0 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N7" smd circle
		(at 0.8 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N8" smd circle
		(at 1.6 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N9" smd circle
		(at 2.4 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P1" smd circle
		(at -4 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P10" smd circle
		(at 3.2 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P11" smd circle
		(at 4 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P2" smd circle
		(at -3.2 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P3" smd circle
		(at -2.4 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P4" smd circle
		(at -1.6 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P5" smd circle
		(at -0.8 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P6" smd circle
		(at 0 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P7" smd circle
		(at 0.8 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P8" smd circle
		(at 1.6 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P9" smd circle
		(at 2.4 3.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R1" smd circle
		(at -4 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R10" smd circle
		(at 3.2 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R11" smd circle
		(at 4 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R2" smd circle
		(at -3.2 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R3" smd circle
		(at -2.4 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R4" smd circle
		(at -1.6 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R5" smd circle
		(at -0.8 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R6" smd circle
		(at 0 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R7" smd circle
		(at 0.8 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R8" smd circle
		(at 1.6 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R9" smd circle
		(at 2.4 4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T1" smd circle
		(at -4 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T10" smd circle
		(at 3.2 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T11" smd circle
		(at 4 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T2" smd circle
		(at -3.2 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T3" smd circle
		(at -2.4 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T4" smd circle
		(at -1.6 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T5" smd circle
		(at -0.8 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T6" smd circle
		(at 0 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T7" smd circle
		(at 0.8 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T8" smd circle
		(at 1.6 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T9" smd circle
		(at 2.4 4.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U1" smd circle
		(at -4 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U10" smd circle
		(at 3.2 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U11" smd circle
		(at 4 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U2" smd circle
		(at -3.2 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U3" smd circle
		(at -2.4 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U4" smd circle
		(at -1.6 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U5" smd circle
		(at -0.8 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U6" smd circle
		(at 0 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U7" smd circle
		(at 0.8 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U8" smd circle
		(at 1.6 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U9" smd circle
		(at 2.4 5.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V1" smd circle
		(at -4 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V10" smd circle
		(at 3.2 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V11" smd circle
		(at 4 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V2" smd circle
		(at -3.2 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V3" smd circle
		(at -2.4 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V4" smd circle
		(at -1.6 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V5" smd circle
		(at -0.8 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V6" smd circle
		(at 0 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V7" smd circle
		(at 0.8 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V8" smd circle
		(at 1.6 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V9" smd circle
		(at 2.4 6.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W1" smd circle
		(at -4 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W10" smd circle
		(at 3.2 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W11" smd circle
		(at 4 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W2" smd circle
		(at -3.2 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W3" smd circle
		(at -2.4 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W4" smd circle
		(at -1.6 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W5" smd circle
		(at -0.8 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W6" smd circle
		(at 0 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W7" smd circle
		(at 0.8 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W8" smd circle
		(at 1.6 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W9" smd circle
		(at 2.4 7.2)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Analog_BGA-209_9.5x16mm_Layout11x19_P0.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
