(footprint "Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Analog BGA-49, 6.25x6.25mm, 49 Ball, 7x7 Layout, 0.8mm Pitch, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-bga/05081600_0_bga49.pdf https://www.analog.com/media/en/technical-documentation/product-information/assembly-considerations-for-umodule-bga-lga-package.pdf")
	(tags "BGA 49 0.8")
	(solder_mask_margin 0.025)
	(solder_paste_margin -0.01)
	(property "Reference" "REF**"
		(at 0 -4.125 0)
		(layer "F.SilkS")
	)
	(property "Value" "Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm"
		(at 0 4.125 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2.4 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -1.6 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.8 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at 0.8 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 1.6 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at 2.4 -2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -2.4 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -1.6 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.8 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at 0.8 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 1.6 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at 2.4 -1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -2.4 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -1.6 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.8 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at 0.8 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 1.6 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at 2.4 -0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -2.4 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -1.6 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.8 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at 0.8 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at 1.6 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D7" smd circle
		(at 2.4 0)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -2.4 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -1.6 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.8 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E5" smd circle
		(at 0.8 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E6" smd circle
		(at 1.6 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E7" smd circle
		(at 2.4 0.8)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -2.4 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -1.6 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.8 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F5" smd circle
		(at 0.8 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at 1.6 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F7" smd circle
		(at 2.4 1.6)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -2.4 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -1.6 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -0.8 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at 0 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G5" smd circle
		(at 0.8 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G6" smd circle
		(at 1.6 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G7" smd circle
		(at 2.4 2.4)
		(size 0.4 0.4)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Analog_BGA-49_6.25x6.25mm_Layout7x7_P0.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
