(footprint "BGA-153_8.0x8.0mm_Layout15x15_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Altera MBGA-153, https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/packaging/04r00471-00.pdf")
	(tags "Altera BGA-153 M153 MBGA")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-153_8.0x8.0mm_Layout15x15_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -3.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -3 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -2.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -1.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -0.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 0.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 1.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at 2.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at 3 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at 3.5 -3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -3.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -3 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -2.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -2 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -1.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -1 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -0.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 0 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 0.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 1 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at 1.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 2 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at 2.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at 3 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at 3.5 -3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.5 -2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -3 -2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 0 -2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at 3 -2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at 3.5 -2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -3 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -2 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -1.5 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -1 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -0.5 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 0 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 0.5 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at 1 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at 1.5 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at 2 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at 3 -2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -3.5 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -3 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -2 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -1.5 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at -1 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at -0.5 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 0 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 0.5 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at 1 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at 1.5 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at 2 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E14" smd circle
		(at 3 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E15" smd circle
		(at 3.5 -1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -3 -1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -2 -1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -1.5 -1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at 1.5 -1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at 2 -1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F14" smd circle
		(at 3 -1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3.5 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -3 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -2 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at -1.5 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at -0.5 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 0 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 0.5 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 1.5 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at 2 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G14" smd circle
		(at 3 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G15" smd circle
		(at 3.5 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -3 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -2.5 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -2 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -1.5 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at -0.5 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 0 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 0.5 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 1.5 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 2 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 2.5 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at 3 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.5 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -3 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -2 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -1.5 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at -0.5 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 0 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 0.5 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 1.5 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 2 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at 3 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J15" smd circle
		(at 3.5 0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -3 1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -2 1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -1.5 1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 1.5 1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at 2 1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at 3 1)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.5 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -3 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -2 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -1.5 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at -1 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at -0.5 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 0 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at 0.5 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at 1 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L11" smd circle
		(at 1.5 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at 2 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L14" smd circle
		(at 3 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L15" smd circle
		(at 3.5 1.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -3 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -2 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M5" smd circle
		(at -1.5 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M6" smd circle
		(at -1 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at -0.5 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at 0 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at 0.5 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M10" smd circle
		(at 1 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M11" smd circle
		(at 1.5 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M12" smd circle
		(at 2 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M14" smd circle
		(at 3 2)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3.5 2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -3 2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 0 2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N14" smd circle
		(at 3 2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N15" smd circle
		(at 3.5 2.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -3.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -3 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -2.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -2 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd circle
		(at -1.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P6" smd circle
		(at -1 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P7" smd circle
		(at -0.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd circle
		(at 0 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd circle
		(at 0.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd circle
		(at 1 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P11" smd circle
		(at 1.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd circle
		(at 2 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P13" smd circle
		(at 2.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P14" smd circle
		(at 3 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P15" smd circle
		(at 3.5 3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -3.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -3 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -2.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R5" smd circle
		(at -1.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R7" smd circle
		(at -0.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R9" smd circle
		(at 0.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R11" smd circle
		(at 1.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R13" smd circle
		(at 2.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R14" smd circle
		(at 3 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R15" smd circle
		(at 3.5 3.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/BGA-153_8.0x8.0mm_Layout15x15_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
