(footprint "BGA-256_11.0x11.0mm_Layout20x20_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Altera MBGA-256, https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/packaging/04r00348-01.pdf")
	(tags "Altera BGA-256 M256 MBGA")
	(property "Reference" "REF**"
		(at 0 -6.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-256_11.0x11.0mm_Layout20x20_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD"
		(at 0 6.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -4.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -4.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -3.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -3.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -2.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -2.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -1.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at -1.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at -0.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -0.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 0.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at 0.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at 1.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at 1.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at 2.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd circle
		(at 2.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd circle
		(at 3.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd circle
		(at 3.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd circle
		(at 4.25 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at 4.75 -4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -4.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -4.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -3.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -3.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -2.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -2.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -1.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -1.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -0.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -0.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at 0.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 0.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at 1.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at 1.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at 2.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at 2.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at 3.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at 3.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at 4.25 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at 4.75 -4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -4.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -4.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -3.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -3.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -2.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at -2.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at -1.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at -1.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at -0.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at -0.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at 0.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at 0.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at 1.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at 1.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at 2.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C16" smd circle
		(at 2.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C17" smd circle
		(at 3.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C18" smd circle
		(at 3.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at 4.25 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C20" smd circle
		(at 4.75 -3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -4.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -4.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -3.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -3.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -2.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -2.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -1.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at -1.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at -0.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at -0.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at 0.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at 0.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at 1.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at 1.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at 2.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at 2.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D17" smd circle
		(at 3.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at 3.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at 4.25 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at 4.75 -3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -4.75 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -4.25 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -3.75 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -3.25 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E17" smd circle
		(at 3.25 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E18" smd circle
		(at 3.75 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E19" smd circle
		(at 4.25 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E20" smd circle
		(at 4.75 -2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -4.75 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -4.25 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -3.75 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -3.25 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F17" smd circle
		(at 3.25 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F18" smd circle
		(at 3.75 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F19" smd circle
		(at 4.25 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F20" smd circle
		(at 4.75 -2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -4.75 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -4.25 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -3.75 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -3.25 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G17" smd circle
		(at 3.25 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G18" smd circle
		(at 3.75 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G19" smd circle
		(at 4.25 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G20" smd circle
		(at 4.75 -1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -4.75 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -4.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -3.75 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -3.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H17" smd circle
		(at 3.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H18" smd circle
		(at 3.75 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at 4.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at 4.75 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -4.75 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -4.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -3.75 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -3.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J17" smd circle
		(at 3.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J18" smd circle
		(at 3.75 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J19" smd circle
		(at 4.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J20" smd circle
		(at 4.75 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -4.75 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -4.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -3.75 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -3.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K17" smd circle
		(at 3.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K18" smd circle
		(at 3.75 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K19" smd circle
		(at 4.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K20" smd circle
		(at 4.75 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -4.75 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -4.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -3.75 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -3.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L17" smd circle
		(at 3.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L18" smd circle
		(at 3.75 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L19" smd circle
		(at 4.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L20" smd circle
		(at 4.75 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -4.75 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -4.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -3.75 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -3.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M17" smd circle
		(at 3.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M18" smd circle
		(at 3.75 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M19" smd circle
		(at 4.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M20" smd circle
		(at 4.75 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -4.75 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -4.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -3.75 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -3.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N17" smd circle
		(at 3.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N18" smd circle
		(at 3.75 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N19" smd circle
		(at 4.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N20" smd circle
		(at 4.75 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -4.75 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -4.25 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -3.75 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -3.25 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P17" smd circle
		(at 3.25 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P18" smd circle
		(at 3.75 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P19" smd circle
		(at 4.25 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P20" smd circle
		(at 4.75 1.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -4.75 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -4.25 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -3.75 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R4" smd circle
		(at -3.25 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R17" smd circle
		(at 3.25 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R18" smd circle
		(at 3.75 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R19" smd circle
		(at 4.25 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R20" smd circle
		(at 4.75 2.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -4.75 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -4.25 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T3" smd circle
		(at -3.75 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T4" smd circle
		(at -3.25 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T17" smd circle
		(at 3.25 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T18" smd circle
		(at 3.75 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T19" smd circle
		(at 4.25 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T20" smd circle
		(at 4.75 2.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -4.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -4.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U3" smd circle
		(at -3.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U4" smd circle
		(at -3.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U5" smd circle
		(at -2.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U6" smd circle
		(at -2.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U7" smd circle
		(at -1.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U8" smd circle
		(at -1.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U9" smd circle
		(at -0.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U10" smd circle
		(at -0.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U11" smd circle
		(at 0.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U12" smd circle
		(at 0.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U13" smd circle
		(at 1.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U14" smd circle
		(at 1.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U15" smd circle
		(at 2.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U16" smd circle
		(at 2.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U17" smd circle
		(at 3.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U18" smd circle
		(at 3.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U19" smd circle
		(at 4.25 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U20" smd circle
		(at 4.75 3.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd circle
		(at -4.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -4.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V3" smd circle
		(at -3.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V4" smd circle
		(at -3.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V5" smd circle
		(at -2.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V6" smd circle
		(at -2.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V7" smd circle
		(at -1.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V8" smd circle
		(at -1.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V9" smd circle
		(at -0.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V10" smd circle
		(at -0.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V11" smd circle
		(at 0.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V12" smd circle
		(at 0.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V13" smd circle
		(at 1.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V14" smd circle
		(at 1.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V15" smd circle
		(at 2.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V16" smd circle
		(at 2.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V17" smd circle
		(at 3.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V18" smd circle
		(at 3.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V19" smd circle
		(at 4.25 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V20" smd circle
		(at 4.75 3.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -4.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W2" smd circle
		(at -4.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W3" smd circle
		(at -3.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W4" smd circle
		(at -3.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W5" smd circle
		(at -2.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W6" smd circle
		(at -2.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W7" smd circle
		(at -1.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W8" smd circle
		(at -1.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W9" smd circle
		(at -0.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W10" smd circle
		(at -0.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W11" smd circle
		(at 0.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W12" smd circle
		(at 0.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W13" smd circle
		(at 1.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W14" smd circle
		(at 1.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W15" smd circle
		(at 2.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W16" smd circle
		(at 2.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W17" smd circle
		(at 3.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W18" smd circle
		(at 3.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W19" smd circle
		(at 4.25 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W20" smd circle
		(at 4.75 4.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y1" smd circle
		(at -4.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -4.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y3" smd circle
		(at -3.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y4" smd circle
		(at -3.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y5" smd circle
		(at -2.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y6" smd circle
		(at -2.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y7" smd circle
		(at -1.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y8" smd circle
		(at -1.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y9" smd circle
		(at -0.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y10" smd circle
		(at -0.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y11" smd circle
		(at 0.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y12" smd circle
		(at 0.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y13" smd circle
		(at 1.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y14" smd circle
		(at 1.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y15" smd circle
		(at 2.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y16" smd circle
		(at 2.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y17" smd circle
		(at 3.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y18" smd circle
		(at 3.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y19" smd circle
		(at 4.25 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y20" smd circle
		(at 4.75 4.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/BGA-256_11.0x11.0mm_Layout20x20_P0.5mm_Ball0.3mm_Pad0.25mm_NSMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
