(footprint "BGA-352_35.0x35.0mm_Layout26x26_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BGA-352, https://www.fujitsu.com/downloads/MICRO/fma/pdfmcu/b352p05.pdf")
	(tags "BGA-352")
	(property "Reference" "REF**"
		(at 0 -18.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-352_35.0x35.0mm_Layout26x26_P1.27mm"
		(at 0 19 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -15.88 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -14.61 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -13.34 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -12.06 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -10.79 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -9.53 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -8.26 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at -6.99 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at -5.71 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -4.45 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at -3.17 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at -1.91 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at -0.64 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at 0.64 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at 1.91 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd circle
		(at 3.17 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd circle
		(at 4.45 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd circle
		(at 5.71 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd circle
		(at 6.99 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at 8.26 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd circle
		(at 9.53 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd circle
		(at 10.79 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at 12.06 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd circle
		(at 13.34 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd circle
		(at 14.61 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd circle
		(at 15.88 -15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd circle
		(at -15.88 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA2" smd circle
		(at -14.61 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA3" smd circle
		(at -13.34 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA4" smd circle
		(at -12.06 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA23" smd circle
		(at 12.06 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA24" smd circle
		(at 13.34 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA25" smd circle
		(at 14.61 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA26" smd circle
		(at 15.88 9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB1" smd circle
		(at -15.88 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -14.61 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB3" smd circle
		(at -13.34 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB4" smd circle
		(at -12.06 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB23" smd circle
		(at 12.06 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB24" smd circle
		(at 13.34 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB25" smd circle
		(at 14.61 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB26" smd circle
		(at 15.88 10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC1" smd circle
		(at -15.88 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC2" smd circle
		(at -14.61 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC3" smd circle
		(at -13.34 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC4" smd circle
		(at -12.06 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC5" smd circle
		(at -10.79 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC6" smd circle
		(at -9.53 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC7" smd circle
		(at -8.26 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC8" smd circle
		(at -6.99 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC9" smd circle
		(at -5.71 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC10" smd circle
		(at -4.45 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC11" smd circle
		(at -3.17 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC12" smd circle
		(at -1.91 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC13" smd circle
		(at -0.64 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC14" smd circle
		(at 0.64 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC15" smd circle
		(at 1.91 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC16" smd circle
		(at 3.17 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC17" smd circle
		(at 4.45 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC18" smd circle
		(at 5.71 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC19" smd circle
		(at 6.99 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC20" smd circle
		(at 8.26 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC21" smd circle
		(at 9.53 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC22" smd circle
		(at 10.79 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC23" smd circle
		(at 12.06 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC24" smd circle
		(at 13.34 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC25" smd circle
		(at 14.61 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC26" smd circle
		(at 15.88 12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD1" smd circle
		(at -15.88 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD2" smd circle
		(at -14.61 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD3" smd circle
		(at -13.34 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD4" smd circle
		(at -12.06 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD5" smd circle
		(at -10.79 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD6" smd circle
		(at -9.53 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD7" smd circle
		(at -8.26 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD8" smd circle
		(at -6.99 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD9" smd circle
		(at -5.71 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD10" smd circle
		(at -4.45 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD11" smd circle
		(at -3.17 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD12" smd circle
		(at -1.91 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD13" smd circle
		(at -0.64 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD14" smd circle
		(at 0.64 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD15" smd circle
		(at 1.91 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD16" smd circle
		(at 3.17 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD17" smd circle
		(at 4.45 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD18" smd circle
		(at 5.71 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD19" smd circle
		(at 6.99 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD20" smd circle
		(at 8.26 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD21" smd circle
		(at 9.53 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD22" smd circle
		(at 10.79 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD23" smd circle
		(at 12.06 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD24" smd circle
		(at 13.34 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD25" smd circle
		(at 14.61 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD26" smd circle
		(at 15.88 13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE1" smd circle
		(at -15.88 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE2" smd circle
		(at -14.61 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE3" smd circle
		(at -13.34 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE4" smd circle
		(at -12.06 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE5" smd circle
		(at -10.79 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE6" smd circle
		(at -9.53 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE7" smd circle
		(at -8.26 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE8" smd circle
		(at -6.99 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE9" smd circle
		(at -5.71 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE10" smd circle
		(at -4.45 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE11" smd circle
		(at -3.17 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE12" smd circle
		(at -1.91 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE13" smd circle
		(at -0.64 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE14" smd circle
		(at 0.64 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE15" smd circle
		(at 1.91 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE16" smd circle
		(at 3.17 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE17" smd circle
		(at 4.45 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE18" smd circle
		(at 5.71 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE19" smd circle
		(at 6.99 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE20" smd circle
		(at 8.26 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE21" smd circle
		(at 9.53 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE22" smd circle
		(at 10.79 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE23" smd circle
		(at 12.06 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE24" smd circle
		(at 13.34 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE25" smd circle
		(at 14.61 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE26" smd circle
		(at 15.88 14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF1" smd circle
		(at -15.88 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF2" smd circle
		(at -14.61 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF3" smd circle
		(at -13.34 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF4" smd circle
		(at -12.06 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF5" smd circle
		(at -10.79 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF6" smd circle
		(at -9.53 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF7" smd circle
		(at -8.26 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF8" smd circle
		(at -6.99 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF9" smd circle
		(at -5.71 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF10" smd circle
		(at -4.45 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF11" smd circle
		(at -3.17 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF12" smd circle
		(at -1.91 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF13" smd circle
		(at -0.64 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF14" smd circle
		(at 0.64 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF15" smd circle
		(at 1.91 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF16" smd circle
		(at 3.17 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF17" smd circle
		(at 4.45 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF18" smd circle
		(at 5.71 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF19" smd circle
		(at 6.99 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF20" smd circle
		(at 8.26 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF21" smd circle
		(at 9.53 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF22" smd circle
		(at 10.79 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF23" smd circle
		(at 12.06 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF24" smd circle
		(at 13.34 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF25" smd circle
		(at 14.61 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF26" smd circle
		(at 15.88 15.88)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -15.88 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -14.61 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -13.34 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -12.06 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -10.79 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -9.53 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -8.26 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -6.99 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -5.71 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -4.45 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at -3.17 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at -1.91 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at -0.64 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at 0.64 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at 1.91 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at 3.17 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at 4.45 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at 5.71 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at 6.99 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at 8.26 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd circle
		(at 9.53 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd circle
		(at 10.79 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd circle
		(at 12.06 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd circle
		(at 13.34 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B25" smd circle
		(at 14.61 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd circle
		(at 15.88 -14.61)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -15.88 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -14.61 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -13.34 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -12.06 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -10.79 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at -9.53 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at -8.26 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at -6.99 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at -5.71 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at -4.45 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at -3.17 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at -1.91 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at -0.64 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at 0.64 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at 1.91 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C16" smd circle
		(at 3.17 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C17" smd circle
		(at 4.45 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C18" smd circle
		(at 5.71 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at 6.99 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C20" smd circle
		(at 8.26 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C21" smd circle
		(at 9.53 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at 10.79 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C23" smd circle
		(at 12.06 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C24" smd circle
		(at 13.34 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C25" smd circle
		(at 14.61 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C26" smd circle
		(at 15.88 -13.34)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -15.88 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -14.61 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -13.34 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -12.06 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -10.79 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -9.53 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -8.26 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at -6.99 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at -5.71 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at -4.45 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -3.17 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at -1.91 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at -0.64 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at 0.64 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at 1.91 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at 3.17 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D17" smd circle
		(at 4.45 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at 5.71 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at 6.99 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at 8.26 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D21" smd circle
		(at 9.53 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D22" smd circle
		(at 10.79 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd circle
		(at 12.06 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D24" smd circle
		(at 13.34 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D25" smd circle
		(at 14.61 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D26" smd circle
		(at 15.88 -12.06)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -15.88 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -14.61 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -13.34 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -12.06 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E23" smd circle
		(at 12.06 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E24" smd circle
		(at 13.34 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E25" smd circle
		(at 14.61 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E26" smd circle
		(at 15.88 -10.79)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -15.88 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -14.61 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -13.34 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -12.06 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F23" smd circle
		(at 12.06 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F24" smd circle
		(at 13.34 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F25" smd circle
		(at 14.61 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F26" smd circle
		(at 15.88 -9.53)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -15.88 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -14.61 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -13.34 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -12.06 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G23" smd circle
		(at 12.06 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G24" smd circle
		(at 13.34 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G25" smd circle
		(at 14.61 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G26" smd circle
		(at 15.88 -8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -15.88 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -14.61 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -13.34 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -12.06 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd circle
		(at 12.06 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H24" smd circle
		(at 13.34 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H25" smd circle
		(at 14.61 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H26" smd circle
		(at 15.88 -6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -15.88 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -14.61 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -13.34 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -12.06 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J23" smd circle
		(at 12.06 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J24" smd circle
		(at 13.34 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J25" smd circle
		(at 14.61 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J26" smd circle
		(at 15.88 -5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -15.88 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -14.61 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -13.34 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -12.06 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K23" smd circle
		(at 12.06 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K24" smd circle
		(at 13.34 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K25" smd circle
		(at 14.61 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K26" smd circle
		(at 15.88 -4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -15.88 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -14.61 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -13.34 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -12.06 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L23" smd circle
		(at 12.06 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L24" smd circle
		(at 13.34 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L25" smd circle
		(at 14.61 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L26" smd circle
		(at 15.88 -3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -15.88 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -14.61 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -13.34 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -12.06 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M23" smd circle
		(at 12.06 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M24" smd circle
		(at 13.34 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M25" smd circle
		(at 14.61 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M26" smd circle
		(at 15.88 -1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -15.88 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -14.61 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -13.34 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -12.06 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N23" smd circle
		(at 12.06 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N24" smd circle
		(at 13.34 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N25" smd circle
		(at 14.61 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N26" smd circle
		(at 15.88 -0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -15.88 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -14.61 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -13.34 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -12.06 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P23" smd circle
		(at 12.06 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P24" smd circle
		(at 13.34 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P25" smd circle
		(at 14.61 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P26" smd circle
		(at 15.88 0.64)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -15.88 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -14.61 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -13.34 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R4" smd circle
		(at -12.06 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R23" smd circle
		(at 12.06 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R24" smd circle
		(at 13.34 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R25" smd circle
		(at 14.61 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R26" smd circle
		(at 15.88 1.91)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -15.88 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -14.61 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T3" smd circle
		(at -13.34 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T4" smd circle
		(at -12.06 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T23" smd circle
		(at 12.06 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T24" smd circle
		(at 13.34 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T25" smd circle
		(at 14.61 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T26" smd circle
		(at 15.88 3.17)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -15.88 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -14.61 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U3" smd circle
		(at -13.34 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U4" smd circle
		(at -12.06 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U23" smd circle
		(at 12.06 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U24" smd circle
		(at 13.34 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U25" smd circle
		(at 14.61 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U26" smd circle
		(at 15.88 4.45)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd circle
		(at -15.88 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -14.61 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V3" smd circle
		(at -13.34 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V4" smd circle
		(at -12.06 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V23" smd circle
		(at 12.06 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V24" smd circle
		(at 13.34 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V25" smd circle
		(at 14.61 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V26" smd circle
		(at 15.88 5.71)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -15.88 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W2" smd circle
		(at -14.61 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W3" smd circle
		(at -13.34 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W4" smd circle
		(at -12.06 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W23" smd circle
		(at 12.06 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W24" smd circle
		(at 13.34 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W25" smd circle
		(at 14.61 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W26" smd circle
		(at 15.88 6.99)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y1" smd circle
		(at -15.88 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -14.61 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y3" smd circle
		(at -13.34 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y4" smd circle
		(at -12.06 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y23" smd circle
		(at 12.06 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y24" smd circle
		(at 13.34 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y25" smd circle
		(at 14.61 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y26" smd circle
		(at 15.88 8.26)
		(size 0.76 0.76)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/BGA-352_35.0x35.0mm_Layout26x26_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
