(footprint "Fujitsu_WLP-15_2.28x3.092mm_Layout3x5_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WLP-15, 3x5 raster, 2.28x3.092mm package, pitch 0.4mm; http://www.fujitsu.com/global/documents/products/devices/semiconductor/fram/lineup/MB85RS1MT-DS501-00022-7v0-E.pdf")
	(tags "BGA 8 0.4")
	(property "Reference" "REF**"
		(at 0 -2.91 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fujitsu_WLP-15_2.28x3.092mm_Layout3x5_P0.4mm"
		(at 0 2.546 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.035)
	(solder_paste_margin 0.000001)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.4 -0.6)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0.4 -0.6)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at 0 -0.3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.4 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0.4 0)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at 0 0.3)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -0.4 0.6)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at 0.4 0.6)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Fujitsu_WLP-15_2.28x3.092mm_Layout3x5_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
