(footprint "ST_TFBGA-257_10x10mm_Layout19x19_P0.5mmP0.65mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ST TFBGA-257, 10.0x10.0mm, 257 Ball, 19x19 Layout, 0.5mm Pitch, https://www.st.com/resource/en/datasheet/stm32mp151a.pdf")
	(tags "BGA 257 0.5")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_TFBGA-257_10x10mm_Layout19x19_P0.5mmP0.65mm"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1A1" smd circle
		(at -2.6 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A2" smd circle
		(at -1.95 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A3" smd circle
		(at -1.3 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A4" smd circle
		(at -0.65 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A5" smd circle
		(at 0 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A6" smd circle
		(at 0.65 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A7" smd circle
		(at 1.3 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A8" smd circle
		(at 1.95 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A9" smd circle
		(at 2.6 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B1" smd circle
		(at -2.6 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B2" smd circle
		(at -1.95 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B3" smd circle
		(at -1.3 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B4" smd circle
		(at -0.65 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B5" smd circle
		(at 0 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B6" smd circle
		(at 0.65 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B7" smd circle
		(at 1.3 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B8" smd circle
		(at 1.95 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B9" smd circle
		(at 2.6 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C1" smd circle
		(at -2.6 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C2" smd circle
		(at -1.95 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C3" smd circle
		(at -1.3 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C4" smd circle
		(at -0.65 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C5" smd circle
		(at 0 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C6" smd circle
		(at 0.65 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C7" smd circle
		(at 1.3 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C8" smd circle
		(at 1.95 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C9" smd circle
		(at 2.6 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D1" smd circle
		(at -2.6 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D2" smd circle
		(at -1.95 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D3" smd circle
		(at -1.3 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D4" smd circle
		(at -0.65 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D5" smd circle
		(at 0 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D6" smd circle
		(at 0.65 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D7" smd circle
		(at 1.3 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D8" smd circle
		(at 1.95 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D9" smd circle
		(at 2.6 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E1" smd circle
		(at -2.6 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E2" smd circle
		(at -1.95 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E3" smd circle
		(at -1.3 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E4" smd circle
		(at -0.65 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E5" smd circle
		(at 0 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E6" smd circle
		(at 0.65 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E7" smd circle
		(at 1.3 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E8" smd circle
		(at 1.95 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E9" smd circle
		(at 2.6 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F1" smd circle
		(at -2.6 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F2" smd circle
		(at -1.95 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F3" smd circle
		(at -1.3 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F4" smd circle
		(at -0.65 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F5" smd circle
		(at 0 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F6" smd circle
		(at 0.65 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F7" smd circle
		(at 1.3 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F8" smd circle
		(at 1.95 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F9" smd circle
		(at 2.6 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G1" smd circle
		(at -2.6 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G2" smd circle
		(at -1.95 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G3" smd circle
		(at -1.3 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G4" smd circle
		(at -0.65 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G5" smd circle
		(at 0 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G6" smd circle
		(at 0.65 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G7" smd circle
		(at 1.3 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G8" smd circle
		(at 1.95 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G9" smd circle
		(at 2.6 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H1" smd circle
		(at -2.6 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H2" smd circle
		(at -1.95 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H3" smd circle
		(at -1.3 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H4" smd circle
		(at -0.65 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H5" smd circle
		(at 0 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H6" smd circle
		(at 0.65 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H7" smd circle
		(at 1.3 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H8" smd circle
		(at 1.95 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H9" smd circle
		(at 2.6 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J1" smd circle
		(at -2.6 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J2" smd circle
		(at -1.95 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J3" smd circle
		(at -1.3 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J4" smd circle
		(at -0.65 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J5" smd circle
		(at 0 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J6" smd circle
		(at 0.65 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J7" smd circle
		(at 1.3 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J8" smd circle
		(at 1.95 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J9" smd circle
		(at 2.6 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A1" smd circle
		(at -4.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A10" smd circle
		(at 0 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A12" smd circle
		(at 1 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A13" smd circle
		(at 1.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A15" smd circle
		(at 2.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A16" smd circle
		(at 3 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A17" smd circle
		(at 3.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A18" smd circle
		(at 4 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A19" smd circle
		(at 4.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -4 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -3.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at -3 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at -2 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at -1.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A9" smd circle
		(at -0.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -4.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B10" smd circle
		(at 0 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B11" smd circle
		(at 0.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B12" smd circle
		(at 1 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B13" smd circle
		(at 1.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B14" smd circle
		(at 2 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B15" smd circle
		(at 2.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B16" smd circle
		(at 3 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B17" smd circle
		(at 3.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B18" smd circle
		(at 4 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B19" smd circle
		(at 4.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -4 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -3.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -3 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at -2.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at -2 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at -1.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at -1 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B9" smd circle
		(at -0.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -4.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C10" smd circle
		(at 0 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C11" smd circle
		(at 0.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C12" smd circle
		(at 1 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C13" smd circle
		(at 1.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C14" smd circle
		(at 2 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C15" smd circle
		(at 2.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C16" smd circle
		(at 3 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C17" smd circle
		(at 3.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C18" smd circle
		(at 4 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C19" smd circle
		(at 4.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -4 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -3.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at -3 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at -2.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at -2 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at -1.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C8" smd circle
		(at -1 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at -0.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -4.5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D17" smd circle
		(at 3.5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D18" smd circle
		(at 4 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D19" smd circle
		(at 4.5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -4 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -3.5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -4.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E17" smd circle
		(at 3.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E18" smd circle
		(at 4 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -4 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -3.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F17" smd circle
		(at 3.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F18" smd circle
		(at 4 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F19" smd circle
		(at 4.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -4 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -3.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -4.5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G17" smd circle
		(at 3.5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G18" smd circle
		(at 4 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G19" smd circle
		(at 4.5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -4 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -3.5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H1" smd circle
		(at -4.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H17" smd circle
		(at 3.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H18" smd circle
		(at 4 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H2" smd circle
		(at -4 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H3" smd circle
		(at -3.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J17" smd circle
		(at 3.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J18" smd circle
		(at 4 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J19" smd circle
		(at 4.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J2" smd circle
		(at -4 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J3" smd circle
		(at -3.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K1" smd circle
		(at -4.5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K17" smd circle
		(at 3.5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K18" smd circle
		(at 4 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K19" smd circle
		(at 4.5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K2" smd circle
		(at -4 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K3" smd circle
		(at -3.5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L1" smd circle
		(at -4.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L17" smd circle
		(at 3.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L18" smd circle
		(at 4 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L2" smd circle
		(at -4 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L3" smd circle
		(at -3.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M17" smd circle
		(at 3.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M18" smd circle
		(at 4 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M19" smd circle
		(at 4.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M2" smd circle
		(at -4 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M3" smd circle
		(at -3.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N1" smd circle
		(at -4.5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N17" smd circle
		(at 3.5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N18" smd circle
		(at 4 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N19" smd circle
		(at 4.5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N2" smd circle
		(at -4 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N3" smd circle
		(at -3.5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P1" smd circle
		(at -4.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P17" smd circle
		(at 3.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P18" smd circle
		(at 4 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P2" smd circle
		(at -4 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P3" smd circle
		(at -3.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R17" smd circle
		(at 3.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R18" smd circle
		(at 4 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R19" smd circle
		(at 4.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R2" smd circle
		(at -4 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R3" smd circle
		(at -3.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T1" smd circle
		(at -4.5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T17" smd circle
		(at 3.5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T18" smd circle
		(at 4 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T19" smd circle
		(at 4.5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T2" smd circle
		(at -4 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T3" smd circle
		(at -3.5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U1" smd circle
		(at -4.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U10" smd circle
		(at 0 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U11" smd circle
		(at 0.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U12" smd circle
		(at 1 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U13" smd circle
		(at 1.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U14" smd circle
		(at 2 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U15" smd circle
		(at 2.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U16" smd circle
		(at 3 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U17" smd circle
		(at 3.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U18" smd circle
		(at 4 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U19" smd circle
		(at 4.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U2" smd circle
		(at -4 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U3" smd circle
		(at -3.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U4" smd circle
		(at -3 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U5" smd circle
		(at -2.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U6" smd circle
		(at -2 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U7" smd circle
		(at -1.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U8" smd circle
		(at -1 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U9" smd circle
		(at -0.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V1" smd circle
		(at -4.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V10" smd circle
		(at 0 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V11" smd circle
		(at 0.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V12" smd circle
		(at 1 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V13" smd circle
		(at 1.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V14" smd circle
		(at 2 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V15" smd circle
		(at 2.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V16" smd circle
		(at 3 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V17" smd circle
		(at 3.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V18" smd circle
		(at 4 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V19" smd circle
		(at 4.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V2" smd circle
		(at -4 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V3" smd circle
		(at -3.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V4" smd circle
		(at -3 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V5" smd circle
		(at -2.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V6" smd circle
		(at -2 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V7" smd circle
		(at -1.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V8" smd circle
		(at -1 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V9" smd circle
		(at -0.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W1" smd circle
		(at -4.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W10" smd circle
		(at 0 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W11" smd circle
		(at 0.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W13" smd circle
		(at 1.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W14" smd circle
		(at 2 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W16" smd circle
		(at 3 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W17" smd circle
		(at 3.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W18" smd circle
		(at 4 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W19" smd circle
		(at 4.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W2" smd circle
		(at -4 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W3" smd circle
		(at -3.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W4" smd circle
		(at -3 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W5" smd circle
		(at -2.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W7" smd circle
		(at -1.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W8" smd circle
		(at -1 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/ST_TFBGA-257_10x10mm_Layout19x19_P0.5mmP0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
