(footprint "ST_TFBGA-361_12x12mm_Layout23x23_P0.5mmP0.65mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ST TFBGA-361, 12.0x12.0mm, 361 Ball, 23x23 Layout, 0.5mm Pitch, https://www.st.com/resource/en/datasheet/stm32mp151a.pdf")
	(tags "BGA 361 0.5")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_TFBGA-361_12x12mm_Layout23x23_P0.5mmP0.65mm"
		(at 0 7 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1A2" smd circle
		(at -1.95 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A3" smd circle
		(at -1.3 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A4" smd circle
		(at -0.65 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A5" smd circle
		(at 0 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A6" smd circle
		(at 0.65 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A7" smd circle
		(at 1.3 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1A8" smd circle
		(at 1.95 -2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B1" smd circle
		(at -2.6 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B2" smd circle
		(at -1.95 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B3" smd circle
		(at -1.3 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B4" smd circle
		(at -0.65 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B5" smd circle
		(at 0 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B6" smd circle
		(at 0.65 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B7" smd circle
		(at 1.3 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B8" smd circle
		(at 1.95 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1B9" smd circle
		(at 2.6 -1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C1" smd circle
		(at -2.6 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C2" smd circle
		(at -1.95 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C3" smd circle
		(at -1.3 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C4" smd circle
		(at -0.65 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C5" smd circle
		(at 0 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C6" smd circle
		(at 0.65 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C7" smd circle
		(at 1.3 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C8" smd circle
		(at 1.95 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1C9" smd circle
		(at 2.6 -1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D1" smd circle
		(at -2.6 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D2" smd circle
		(at -1.95 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D3" smd circle
		(at -1.3 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D4" smd circle
		(at -0.65 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D5" smd circle
		(at 0 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D6" smd circle
		(at 0.65 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D7" smd circle
		(at 1.3 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D8" smd circle
		(at 1.95 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1D9" smd circle
		(at 2.6 -0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E1" smd circle
		(at -2.6 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E2" smd circle
		(at -1.95 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E3" smd circle
		(at -1.3 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E4" smd circle
		(at -0.65 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E5" smd circle
		(at 0 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E6" smd circle
		(at 0.65 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E7" smd circle
		(at 1.3 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E8" smd circle
		(at 1.95 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1E9" smd circle
		(at 2.6 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F1" smd circle
		(at -2.6 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F2" smd circle
		(at -1.95 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F3" smd circle
		(at -1.3 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F4" smd circle
		(at -0.65 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F5" smd circle
		(at 0 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F6" smd circle
		(at 0.65 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F7" smd circle
		(at 1.3 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F8" smd circle
		(at 1.95 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1F9" smd circle
		(at 2.6 0.65)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G1" smd circle
		(at -2.6 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G2" smd circle
		(at -1.95 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G3" smd circle
		(at -1.3 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G4" smd circle
		(at -0.65 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G5" smd circle
		(at 0 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G6" smd circle
		(at 0.65 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G7" smd circle
		(at 1.3 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G8" smd circle
		(at 1.95 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1G9" smd circle
		(at 2.6 1.3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H1" smd circle
		(at -2.6 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H2" smd circle
		(at -1.95 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H3" smd circle
		(at -1.3 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H4" smd circle
		(at -0.65 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H5" smd circle
		(at 0 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H6" smd circle
		(at 0.65 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H7" smd circle
		(at 1.3 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H8" smd circle
		(at 1.95 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1H9" smd circle
		(at 2.6 1.95)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J2" smd circle
		(at -1.95 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J3" smd circle
		(at -1.3 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J4" smd circle
		(at -0.65 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J5" smd circle
		(at 0 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J6" smd circle
		(at 0.65 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J7" smd circle
		(at 1.3 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1J8" smd circle
		(at 1.95 2.6)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A1" smd circle
		(at -5.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A10" smd circle
		(at -1 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A11" smd circle
		(at -0.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A13" smd circle
		(at 0.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A14" smd circle
		(at 1 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A16" smd circle
		(at 2 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A17" smd circle
		(at 2.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A19" smd circle
		(at 3.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A20" smd circle
		(at 4 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A21" smd circle
		(at 4.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A22" smd circle
		(at 5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A23" smd circle
		(at 5.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -4.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at -4 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at -3.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at -2.5 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A8" smd circle
		(at -2 -5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA1" smd circle
		(at -5.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA10" smd circle
		(at -1 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA11" smd circle
		(at -0.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA12" smd circle
		(at 0 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA13" smd circle
		(at 0.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA14" smd circle
		(at 1 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA15" smd circle
		(at 1.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA16" smd circle
		(at 2 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA17" smd circle
		(at 2.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA18" smd circle
		(at 3 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA19" smd circle
		(at 3.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA2" smd circle
		(at -5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA20" smd circle
		(at 4 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA21" smd circle
		(at 4.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA22" smd circle
		(at 5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA23" smd circle
		(at 5.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA3" smd circle
		(at -4.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA4" smd circle
		(at -4 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA5" smd circle
		(at -3.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA6" smd circle
		(at -3 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA7" smd circle
		(at -2.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA8" smd circle
		(at -2 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AA9" smd circle
		(at -1.5 4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB1" smd circle
		(at -5.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB10" smd circle
		(at -1 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB11" smd circle
		(at -0.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB12" smd circle
		(at 0 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB13" smd circle
		(at 0.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB14" smd circle
		(at 1 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB15" smd circle
		(at 1.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB16" smd circle
		(at 2 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB17" smd circle
		(at 2.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB18" smd circle
		(at 3 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB19" smd circle
		(at 3.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB2" smd circle
		(at -5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB20" smd circle
		(at 4 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB21" smd circle
		(at 4.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB22" smd circle
		(at 5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB23" smd circle
		(at 5.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB3" smd circle
		(at -4.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB4" smd circle
		(at -4 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB5" smd circle
		(at -3.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB6" smd circle
		(at -3 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB7" smd circle
		(at -2.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB8" smd circle
		(at -2 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AB9" smd circle
		(at -1.5 5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC1" smd circle
		(at -5.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC10" smd circle
		(at -1 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC11" smd circle
		(at -0.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC13" smd circle
		(at 0.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC14" smd circle
		(at 1 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC16" smd circle
		(at 2 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC17" smd circle
		(at 2.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC19" smd circle
		(at 3.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC2" smd circle
		(at -5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC20" smd circle
		(at 4 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC21" smd circle
		(at 4.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC22" smd circle
		(at 5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC23" smd circle
		(at 5.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC3" smd circle
		(at -4.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC4" smd circle
		(at -4 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC5" smd circle
		(at -3.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC7" smd circle
		(at -2.5 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "AC8" smd circle
		(at -2 5.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -5.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B10" smd circle
		(at -1 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B11" smd circle
		(at -0.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B12" smd circle
		(at 0 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B13" smd circle
		(at 0.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B14" smd circle
		(at 1 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B15" smd circle
		(at 1.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B16" smd circle
		(at 2 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B17" smd circle
		(at 2.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B18" smd circle
		(at 3 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B19" smd circle
		(at 3.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B20" smd circle
		(at 4 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B21" smd circle
		(at 4.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B22" smd circle
		(at 5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B23" smd circle
		(at 5.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -4.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -4 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at -3.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at -3 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at -2.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at -2 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B9" smd circle
		(at -1.5 -5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -5.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C10" smd circle
		(at -1 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C11" smd circle
		(at -0.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C12" smd circle
		(at 0 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C13" smd circle
		(at 0.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C14" smd circle
		(at 1 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C15" smd circle
		(at 1.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C16" smd circle
		(at 2 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C17" smd circle
		(at 2.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C18" smd circle
		(at 3 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C19" smd circle
		(at 3.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C20" smd circle
		(at 4 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C21" smd circle
		(at 4.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C22" smd circle
		(at 5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C23" smd circle
		(at 5.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -4.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at -4 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at -3.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at -3 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at -2.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C8" smd circle
		(at -2 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at -1.5 -4.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -5.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D10" smd circle
		(at -1 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D11" smd circle
		(at -0.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D12" smd circle
		(at 0 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D13" smd circle
		(at 0.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D14" smd circle
		(at 1 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D15" smd circle
		(at 1.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D16" smd circle
		(at 2 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D17" smd circle
		(at 2.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D18" smd circle
		(at 3 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D19" smd circle
		(at 3.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D20" smd circle
		(at 4 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D21" smd circle
		(at 4.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D22" smd circle
		(at 5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D23" smd circle
		(at 5.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -4.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at -4 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at -3.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at -3 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D7" smd circle
		(at -2.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D8" smd circle
		(at -2 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D9" smd circle
		(at -1.5 -4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -5.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E20" smd circle
		(at 4 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E21" smd circle
		(at 4.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E22" smd circle
		(at 5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E23" smd circle
		(at 5.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -4.5 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at -4 -3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F20" smd circle
		(at 4 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F21" smd circle
		(at 4.5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F22" smd circle
		(at 5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -4.5 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at -4 -3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -5.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G20" smd circle
		(at 4 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G21" smd circle
		(at 4.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G22" smd circle
		(at 5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G23" smd circle
		(at 5.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -4.5 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at -4 -2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H1" smd circle
		(at -5.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H2" smd circle
		(at -5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H20" smd circle
		(at 4 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H21" smd circle
		(at 4.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H22" smd circle
		(at 5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H23" smd circle
		(at 5.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H3" smd circle
		(at -4.5 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H4" smd circle
		(at -4 -2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J2" smd circle
		(at -5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J20" smd circle
		(at 4 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J21" smd circle
		(at 4.5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J22" smd circle
		(at 5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J3" smd circle
		(at -4.5 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J4" smd circle
		(at -4 -1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K1" smd circle
		(at -5.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K2" smd circle
		(at -5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K20" smd circle
		(at 4 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K21" smd circle
		(at 4.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K22" smd circle
		(at 5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K23" smd circle
		(at 5.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K3" smd circle
		(at -4.5 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K4" smd circle
		(at -4 -1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L1" smd circle
		(at -5.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L2" smd circle
		(at -5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L20" smd circle
		(at 4 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L21" smd circle
		(at 4.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L22" smd circle
		(at 5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L23" smd circle
		(at 5.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L3" smd circle
		(at -4.5 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L4" smd circle
		(at -4 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M2" smd circle
		(at -5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M20" smd circle
		(at 4 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M21" smd circle
		(at 4.5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M22" smd circle
		(at 5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M3" smd circle
		(at -4.5 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M4" smd circle
		(at -4 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N1" smd circle
		(at -5.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N2" smd circle
		(at -5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N20" smd circle
		(at 4 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N21" smd circle
		(at 4.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N22" smd circle
		(at 5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N23" smd circle
		(at 5.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N3" smd circle
		(at -4.5 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N4" smd circle
		(at -4 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P1" smd circle
		(at -5.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P2" smd circle
		(at -5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P20" smd circle
		(at 4 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P21" smd circle
		(at 4.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P22" smd circle
		(at 5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P23" smd circle
		(at 5.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P3" smd circle
		(at -4.5 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P4" smd circle
		(at -4 1)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R2" smd circle
		(at -5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R20" smd circle
		(at 4 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R21" smd circle
		(at 4.5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R22" smd circle
		(at 5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R3" smd circle
		(at -4.5 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R4" smd circle
		(at -4 1.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T1" smd circle
		(at -5.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T2" smd circle
		(at -5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T20" smd circle
		(at 4 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T21" smd circle
		(at 4.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T22" smd circle
		(at 5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T23" smd circle
		(at 5.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T3" smd circle
		(at -4.5 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T4" smd circle
		(at -4 2)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U1" smd circle
		(at -5.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U2" smd circle
		(at -5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U20" smd circle
		(at 4 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U21" smd circle
		(at 4.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U22" smd circle
		(at 5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U23" smd circle
		(at 5.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U3" smd circle
		(at -4.5 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U4" smd circle
		(at -4 2.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V2" smd circle
		(at -5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V20" smd circle
		(at 4 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V21" smd circle
		(at 4.5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V22" smd circle
		(at 5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V3" smd circle
		(at -4.5 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V4" smd circle
		(at -4 3)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W1" smd circle
		(at -5.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W2" smd circle
		(at -5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W20" smd circle
		(at 4 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W21" smd circle
		(at 4.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W22" smd circle
		(at 5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W23" smd circle
		(at 5.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W3" smd circle
		(at -4.5 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W4" smd circle
		(at -4 3.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y1" smd circle
		(at -5.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y10" smd circle
		(at -1 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y11" smd circle
		(at -0.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y12" smd circle
		(at 0 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y13" smd circle
		(at 0.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y14" smd circle
		(at 1 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y15" smd circle
		(at 1.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y16" smd circle
		(at 2 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y17" smd circle
		(at 2.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y18" smd circle
		(at 3 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y19" smd circle
		(at 3.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y2" smd circle
		(at -5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y20" smd circle
		(at 4 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y21" smd circle
		(at 4.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y22" smd circle
		(at 5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y23" smd circle
		(at 5.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y3" smd circle
		(at -4.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y4" smd circle
		(at -4 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y5" smd circle
		(at -3.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y6" smd circle
		(at -3 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y7" smd circle
		(at -2.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y8" smd circle
		(at -2 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "Y9" smd circle
		(at -1.5 4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/ST_TFBGA-361_12x12mm_Layout23x23_P0.5mmP0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
