(footprint "ST_uTFBGA-36_3.6x3.6mm_Layout6x6_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ST uTFBGA-36, 0.25mm pad, 3.6x3.6mm, 36 Ball, 6x6 Layout, 0.5mm Pitch, https://www.st.com/resource/en/datasheet/stulpi01a.pdf")
	(tags "BGA 36 0.5")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_uTFBGA-36_3.6x3.6mm_Layout6x6_P0.5mm"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -0.75 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at 0.75 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 1.25 -1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -1.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -0.75 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at 0.75 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 1.25 -0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -1.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -0.75 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at 0.75 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 1.25 -0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -1.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -0.75 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at 0.75 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at 1.25 0.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -1.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -0.75 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E5" smd circle
		(at 0.75 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E6" smd circle
		(at 1.25 0.75)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -1.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -0.75 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F5" smd circle
		(at 0.75 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at 1.25 1.25)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/ST_uTFBGA-36_3.6x3.6mm_Layout6x6_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
