(footprint "Texas_DSBGA-16_2.39x2.39mm_Layout4x4_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, area grid, YZF, YZF0016, 2.39x2.39mm, 16 Ball, 4x4 Layout, 0.5mm Pitch, https://www.ti.com/lit/ds/symlink/dac80508.pdf")
	(tags "BGA 16 0.5")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-16_2.39x2.39mm_Layout4x4_P0.5mm"
		(at 0 2.195 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.75 -0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.75 -0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.75 0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.75 0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.25 -0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.25 -0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.25 0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at -0.25 0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.25 -0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.25 -0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.25 0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.25 0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.75 -0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.75 -0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.75 0.25)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "" smd roundrect
		(at 0.75 0.75)
		(size 0.25 0.25)
		(layers "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "A1" smd circle
		(at -0.75 -0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A2" smd circle
		(at -0.25 -0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A3" smd circle
		(at 0.25 -0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.75 -0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.75 -0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" smd circle
		(at -0.25 -0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" smd circle
		(at 0.25 -0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.75 -0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.75 0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C2" smd circle
		(at -0.25 0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C3" smd circle
		(at 0.25 0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.75 0.25)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D1" smd circle
		(at -0.75 0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D2" smd circle
		(at -0.25 0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D3" smd circle
		(at 0.25 0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.75 0.75)
		(size 0.245 0.245)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-16_2.39x2.39mm_Layout4x4_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
