(footprint "Texas_DSBGA-28_1.9x3mm_Layout4x7_P0.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, area grid, 1.9x3.0mm, 28 Ball, 4x7 Layout, 0.4mm Pitch, http://www.ti.com/lit/ds/symlink/bq51050b.pdf, http://www.ti.com/lit/an/snva009ag/snva009ag.pdf")
	(tags "BGA 28 0.4 TI 28-ball YFP R-XBGA-N28")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-28_1.9x3mm_Layout4x7_P0.4mm"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.6 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -0.2 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at 0.2 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.6 -1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.6 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -0.2 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at 0.2 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.6 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.6 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -0.2 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at 0.2 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.6 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -0.6 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -0.2 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at 0.2 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.6 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -0.6 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -0.2 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at 0.2 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0.6 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -0.6 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -0.2 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at 0.2 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0.6 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -0.6 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -0.2 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at 0.2 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at 0.6 1.2)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-28_1.9x3mm_Layout4x7_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
