(footprint "Texas_DSBGA-5_0.8875x1.3875mm_Layout2x3_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, area grid, NSMD, YZP0005 pad definition, 0.8875x1.3875mm, 5 Ball, 2x3 Layout, 0.5mm Pitch, https://www.ti.com/lit/ds/symlink/sn74lvc1g17.pdf#page=42, https://www.ti.com/lit/ml/mxbg018l/mxbg018l.pdf")
	(tags "BGA 5 0.5 YZP")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -1.69375 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-5_0.8875x1.3875mm_Layout2x3_P0.5mm"
		(at 0 1.69375 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.25 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0.25 -0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.25 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.25 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at 0.25 0.5)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-5_0.8875x1.3875mm_Layout2x3_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
