(footprint "Texas_DSBGA-6_0.855x1.255mm_Layout2x3_P0.4mm_LevelB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, area grid, YBG pad definition, 0.95x1.488mm, 6 Ball, 2x3 Layout, 0.4mm Pitch, YFF0006, NSMD pad definition,  https://www.ti.com/lit/ds/symlink/lmg1020.pdf, https://www.ti.com/lit/ml/mxbg078z/mxbg078z.pdf")
	(tags "BGA 6 0.4 YFF0006")
	(property "Reference" "REF**"
		(at 0.35 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-6_0.855x1.255mm_Layout2x3_P0.4mm_LevelB"
		(at 0 1.744 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.2 -0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0.2 -0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.2 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" smd circle
		(at 0.2 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.2 0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C2" smd circle
		(at 0.2 0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-6_0.855x1.255mm_Layout2x3_P0.4mm_LevelB.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
