(footprint "Texas_DSBGA-8_0.705x1.468mm_Layout2x4_P0.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, area grid, NSMD, YBJ0008 pad definition, 0.705x1.468mm, 8 Ball, 2x4 Layout, 0.4mm Pitch, https://www.ti.com/lit/gpn/ina234")
	(tags "BGA 8 0.4")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -1.734 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-8_0.705x1.468mm_Layout2x4_P0.4mm"
		(at 0 1.734 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.2 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0.2 -0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.2 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at 0.2 -0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.2 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at 0.2 0.2)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -0.2 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at 0.2 0.6)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-8_0.705x1.468mm_Layout2x4_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
