(footprint "Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, 0.9x1.9mm, 8 bump 2x4 (perimeter) array, NSMD pad definition (http://www.ti.com/lit/ds/symlink/txb0102.pdf, http://www.ti.com/lit/an/snva009ag/snva009ag.pdf)")
	(tags "Texas Instruments DSBGA BGA YZP R-XBGA-N8")
	(property "Reference" "REF**"
		(at 0 -2.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.25 0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.25 0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
	)
	(pad "A1" smd circle
		(at -0.25 -0.75)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0.25 -0.75)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.25 -0.25)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" smd circle
		(at 0.25 -0.25)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.25 0.25)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "C2" smd circle
		(at 0.25 0.25)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D1" smd circle
		(at -0.25 0.75)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(pad "D2" smd circle
		(at 0.25 0.75)
		(size 0.265 0.265)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
