(footprint "Texas_DSBGA-8_1.5195x1.5195mm_Layout3x3_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, area grid, YZR pad definition, 1.5195x1.5195mm, 8 Ball, 3x3 Layout, 0.5mm Pitch, http://www.ti.com/lit/ml/mxbg270/mxbg270.pdf")
	(tags "BGA 8 0.5")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -1.75975 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-8_1.5195x1.5195mm_Layout3x3_P0.5mm"
		(at 0 1.75975 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.5 -0.5)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at 0 -0.5)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at 0.5 -0.5)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.5 0)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at 0.5 0)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.5 0.5)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at 0 0.5)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at 0.5 0.5)
		(size 0.2625 0.2625)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-8_1.5195x1.5195mm_Layout3x3_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
