(footprint "Texas_MicroStar_Junior_BGA-12_2.0x2.5mm_Layout4x3_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, BGA Microstar Junior, 2x2.5mm, 12 bump 4x3 grid, NSMD pad definition (http://www.ti.com/lit/ds/symlink/txb0104.pdf, http://www.ti.com/lit/wp/ssyz015b/ssyz015b.pdf)")
	(tags "Texas_Junior_BGA-12")
	(property "Reference" "REF**"
		(at -0.25 -2.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_MicroStar_Junior_BGA-12_2.0x2.5mm_Layout4x3_P0.5mm"
		(at 0.25 2.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.75 -0.5)
		(size 0.25 0.25)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.25 -0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0.25 -0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0.75 -0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.75 0)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -0.25 0)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at 0.25 0)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0.75 0)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.75 0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.25 0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0.25 0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0.75 0.5)
		(size 0.3 0.3)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_MicroStar_Junior_BGA-12_2.0x2.5mm_Layout4x3_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
