(footprint "Texas_YFP0020_DSBGA-20_1.588x1.988mm_Layout4x5_P0.4mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas Instruments, YFP0020, DSBGA-20, area grid, 1.588x1.988mm, 20 Ball, 4x5 Layout, 0.4mm Pitch, https://www.ti.com/lit/ds/symlink/txs0206.pdf")
	(tags "BGA 20 0.4")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -1.994 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_YFP0020_DSBGA-20_1.588x1.988mm_Layout4x5_P0.4mm"
		(at 0 1.994 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.6 -0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -0.2 -0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at 0.2 -0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.6 -0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -0.6 -0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -0.2 -0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at 0.2 -0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.6 -0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -0.6 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -0.2 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at 0.2 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.6 0)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -0.6 0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -0.2 0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at 0.2 0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.6 0.4)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -0.6 0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -0.2 0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at 0.2 0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0.6 0.8)
		(size 0.23 0.23)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_YFP0020_DSBGA-20_1.588x1.988mm_Layout4x5_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
