(footprint "UFBGA-132_7x7mm_Layout12x12_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "UFBGA-132, 7.0x7.0mm, 132 Ball, 12x12 Layout, 0.5mm Pitch, http://www.st.com/resource/en/datasheet/stm32l152zc.pdf#page=123")
	(tags "BGA 132 0.5")
	(solder_mask_margin 0.04)
	(solder_paste_margin 0.000001)
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "UFBGA-132_7x7mm_Layout12x12_P0.5mm"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2.75 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A10" smd circle
		(at 1.75 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A11" smd circle
		(at 2.25 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A12" smd circle
		(at 2.75 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -2.25 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -1.75 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at -1.25 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at -0.75 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at -0.25 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at 0.25 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A8" smd circle
		(at 0.75 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A9" smd circle
		(at 1.25 -2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -2.75 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B10" smd circle
		(at 1.75 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B11" smd circle
		(at 2.25 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B12" smd circle
		(at 2.75 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -2.25 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -1.75 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -1.25 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at -0.75 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at -0.25 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at 0.25 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at 0.75 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B9" smd circle
		(at 1.25 -2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -2.75 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C10" smd circle
		(at 1.75 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C11" smd circle
		(at 2.25 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C12" smd circle
		(at 2.75 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -2.25 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -1.75 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at -1.25 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at -0.75 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at -0.25 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at 0.25 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C8" smd circle
		(at 0.75 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at 1.25 -1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -2.75 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D10" smd circle
		(at 1.75 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D11" smd circle
		(at 2.25 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D12" smd circle
		(at 2.75 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -2.25 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -1.75 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at -1.25 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at -0.75 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at -0.25 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D7" smd circle
		(at 0.25 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D8" smd circle
		(at 0.75 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D9" smd circle
		(at 1.25 -1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -2.75 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E10" smd circle
		(at 1.75 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E11" smd circle
		(at 2.25 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E12" smd circle
		(at 2.75 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -2.25 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -1.75 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at -1.25 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E9" smd circle
		(at 1.25 -0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -2.75 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F10" smd circle
		(at 1.75 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F11" smd circle
		(at 2.25 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F12" smd circle
		(at 2.75 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -2.25 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -1.75 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at -1.25 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at -0.25 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F7" smd circle
		(at 0.25 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F9" smd circle
		(at 1.25 -0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -2.75 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G10" smd circle
		(at 1.75 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G11" smd circle
		(at 2.25 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G12" smd circle
		(at 2.75 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -2.25 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -1.75 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G4" smd circle
		(at -1.25 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G6" smd circle
		(at -0.25 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G7" smd circle
		(at 0.25 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G9" smd circle
		(at 1.25 0.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H1" smd circle
		(at -2.75 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H10" smd circle
		(at 1.75 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H11" smd circle
		(at 2.25 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H12" smd circle
		(at 2.75 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H2" smd circle
		(at -2.25 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H3" smd circle
		(at -1.75 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H4" smd circle
		(at -1.25 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H9" smd circle
		(at 1.25 0.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J1" smd circle
		(at -2.75 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J10" smd circle
		(at 1.75 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J11" smd circle
		(at 2.25 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J12" smd circle
		(at 2.75 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J2" smd circle
		(at -2.25 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J3" smd circle
		(at -1.75 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J4" smd circle
		(at -1.25 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J5" smd circle
		(at -0.75 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J6" smd circle
		(at -0.25 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J7" smd circle
		(at 0.25 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J8" smd circle
		(at 0.75 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J9" smd circle
		(at 1.25 1.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K1" smd circle
		(at -2.75 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K10" smd circle
		(at 1.75 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K11" smd circle
		(at 2.25 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K12" smd circle
		(at 2.75 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K2" smd circle
		(at -2.25 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K3" smd circle
		(at -1.75 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K4" smd circle
		(at -1.25 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K5" smd circle
		(at -0.75 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K6" smd circle
		(at -0.25 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K7" smd circle
		(at 0.25 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K8" smd circle
		(at 0.75 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K9" smd circle
		(at 1.25 1.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L1" smd circle
		(at -2.75 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L10" smd circle
		(at 1.75 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L11" smd circle
		(at 2.25 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L12" smd circle
		(at 2.75 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L2" smd circle
		(at -2.25 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L3" smd circle
		(at -1.75 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L4" smd circle
		(at -1.25 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L5" smd circle
		(at -0.75 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L6" smd circle
		(at -0.25 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L7" smd circle
		(at 0.25 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L8" smd circle
		(at 0.75 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L9" smd circle
		(at 1.25 2.25)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M1" smd circle
		(at -2.75 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M10" smd circle
		(at 1.75 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M11" smd circle
		(at 2.25 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M12" smd circle
		(at 2.75 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M2" smd circle
		(at -2.25 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M3" smd circle
		(at -1.75 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M4" smd circle
		(at -1.25 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M5" smd circle
		(at -0.75 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M6" smd circle
		(at -0.25 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M7" smd circle
		(at 0.25 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M8" smd circle
		(at 0.75 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M9" smd circle
		(at 1.25 2.75)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/UFBGA-132_7x7mm_Layout12x12_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
