(footprint "Xilinx_CPG236"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Artix-7 BGA, NSMD pad definition Appendix A, 10x10mm, 238 Ball, 19x19 Layout, 0.5mm Pitch, https://www.xilinx.com/support/documentation/user_guides/ug475_7Series_Pkg_Pinout.pdf#page=266")
	(tags "BGA 238 0.5 C P 2 3 6   C P G 2 3 6")
	(solder_mask_margin 0.05)
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Xilinx_CPG236"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -4.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A10" smd circle
		(at 0 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A11" smd circle
		(at 0.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A12" smd circle
		(at 1 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A13" smd circle
		(at 1.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A14" smd circle
		(at 2 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A15" smd circle
		(at 2.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A16" smd circle
		(at 3 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A17" smd circle
		(at 3.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A18" smd circle
		(at 4 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A19" smd circle
		(at 4.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -4 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -3.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at -3 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at -2.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at -2 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at -1.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A8" smd circle
		(at -1 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A9" smd circle
		(at -0.5 -4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -4.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B10" smd circle
		(at 0 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B11" smd circle
		(at 0.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B12" smd circle
		(at 1 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B13" smd circle
		(at 1.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B14" smd circle
		(at 2 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B15" smd circle
		(at 2.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B16" smd circle
		(at 3 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B17" smd circle
		(at 3.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B18" smd circle
		(at 4 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B19" smd circle
		(at 4.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -4 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -3.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -3 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at -2.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at -2 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B7" smd circle
		(at -1.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at -1 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B9" smd circle
		(at -0.5 -4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -4.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C10" smd circle
		(at 0 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C11" smd circle
		(at 0.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C12" smd circle
		(at 1 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C13" smd circle
		(at 1.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C14" smd circle
		(at 2 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C15" smd circle
		(at 2.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C16" smd circle
		(at 3 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C17" smd circle
		(at 3.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C18" smd circle
		(at 4 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C19" smd circle
		(at 4.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -4 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -3.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at -3 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at -2.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at -2 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at -1.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C8" smd circle
		(at -1 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at -0.5 -3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -4.5 -3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D17" smd circle
		(at 3.5 -3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D18" smd circle
		(at 4 -3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D19" smd circle
		(at 4.5 -3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -4 -3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -3.5 -3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -4.5 -2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E17" smd circle
		(at 3.5 -2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E18" smd circle
		(at 4 -2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E19" smd circle
		(at 4.5 -2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -4 -2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -3.5 -2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -4.5 -2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F17" smd circle
		(at 3.5 -2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F18" smd circle
		(at 4 -2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F19" smd circle
		(at 4.5 -2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -4 -2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -3.5 -2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G1" smd circle
		(at -4.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G10" smd circle
		(at 0 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G11" smd circle
		(at 0.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G12" smd circle
		(at 1 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G13" smd circle
		(at 1.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G17" smd circle
		(at 3.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G18" smd circle
		(at 4 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G19" smd circle
		(at 4.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G2" smd circle
		(at -4 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G3" smd circle
		(at -3.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G7" smd circle
		(at -1.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G8" smd circle
		(at -1 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "G9" smd circle
		(at -0.5 -1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H1" smd circle
		(at -4.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H10" smd circle
		(at 0 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H11" smd circle
		(at 0.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H12" smd circle
		(at 1 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H13" smd circle
		(at 1.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H17" smd circle
		(at 3.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H18" smd circle
		(at 4 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H19" smd circle
		(at 4.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H2" smd circle
		(at -4 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H3" smd circle
		(at -3.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H7" smd circle
		(at -1.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H8" smd circle
		(at -1 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "H9" smd circle
		(at -0.5 -1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J1" smd circle
		(at -4.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J10" smd circle
		(at 0 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J11" smd circle
		(at 0.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J12" smd circle
		(at 1 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J13" smd circle
		(at 1.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J17" smd circle
		(at 3.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J18" smd circle
		(at 4 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J19" smd circle
		(at 4.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J2" smd circle
		(at -4 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J3" smd circle
		(at -3.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J7" smd circle
		(at -1.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J8" smd circle
		(at -1 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "J9" smd circle
		(at -0.5 -0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K1" smd circle
		(at -4.5 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K12" smd circle
		(at 1 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K13" smd circle
		(at 1.5 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K17" smd circle
		(at 3.5 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K18" smd circle
		(at 4 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K19" smd circle
		(at 4.5 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K2" smd circle
		(at -4 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K3" smd circle
		(at -3.5 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K7" smd circle
		(at -1.5 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "K8" smd circle
		(at -1 0)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L1" smd circle
		(at -4.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L10" smd circle
		(at 0 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L11" smd circle
		(at 0.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L12" smd circle
		(at 1 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L13" smd circle
		(at 1.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L17" smd circle
		(at 3.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L18" smd circle
		(at 4 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L19" smd circle
		(at 4.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L2" smd circle
		(at -4 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L3" smd circle
		(at -3.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L7" smd circle
		(at -1.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L8" smd circle
		(at -1 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "L9" smd circle
		(at -0.5 0.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M1" smd circle
		(at -4.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M10" smd circle
		(at 0 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M11" smd circle
		(at 0.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M12" smd circle
		(at 1 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M13" smd circle
		(at 1.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M17" smd circle
		(at 3.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M18" smd circle
		(at 4 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M19" smd circle
		(at 4.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M2" smd circle
		(at -4 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M3" smd circle
		(at -3.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M7" smd circle
		(at -1.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M8" smd circle
		(at -1 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "M9" smd circle
		(at -0.5 1)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N1" smd circle
		(at -4.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N10" smd circle
		(at 0 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N11" smd circle
		(at 0.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N12" smd circle
		(at 1 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N13" smd circle
		(at 1.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N17" smd circle
		(at 3.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N18" smd circle
		(at 4 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N19" smd circle
		(at 4.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N2" smd circle
		(at -4 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N3" smd circle
		(at -3.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N7" smd circle
		(at -1.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N8" smd circle
		(at -1 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "N9" smd circle
		(at -0.5 1.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P1" smd circle
		(at -4.5 2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P17" smd circle
		(at 3.5 2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P18" smd circle
		(at 4 2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P19" smd circle
		(at 4.5 2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P2" smd circle
		(at -4 2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "P3" smd circle
		(at -3.5 2)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R1" smd circle
		(at -4.5 2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R17" smd circle
		(at 3.5 2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R18" smd circle
		(at 4 2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R19" smd circle
		(at 4.5 2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R2" smd circle
		(at -4 2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "R3" smd circle
		(at -3.5 2.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T1" smd circle
		(at -4.5 3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T17" smd circle
		(at 3.5 3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T18" smd circle
		(at 4 3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T19" smd circle
		(at 4.5 3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T2" smd circle
		(at -4 3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "T3" smd circle
		(at -3.5 3)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U1" smd circle
		(at -4.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U10" smd circle
		(at 0 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U11" smd circle
		(at 0.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U12" smd circle
		(at 1 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U13" smd circle
		(at 1.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U14" smd circle
		(at 2 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U15" smd circle
		(at 2.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U16" smd circle
		(at 3 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U17" smd circle
		(at 3.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U18" smd circle
		(at 4 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U19" smd circle
		(at 4.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U2" smd circle
		(at -4 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U3" smd circle
		(at -3.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U4" smd circle
		(at -3 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U5" smd circle
		(at -2.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U6" smd circle
		(at -2 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U7" smd circle
		(at -1.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U8" smd circle
		(at -1 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "U9" smd circle
		(at -0.5 3.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V1" smd circle
		(at -4.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V10" smd circle
		(at 0 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V11" smd circle
		(at 0.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V12" smd circle
		(at 1 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V13" smd circle
		(at 1.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V14" smd circle
		(at 2 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V15" smd circle
		(at 2.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V16" smd circle
		(at 3 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V17" smd circle
		(at 3.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V18" smd circle
		(at 4 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V19" smd circle
		(at 4.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V2" smd circle
		(at -4 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V3" smd circle
		(at -3.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V4" smd circle
		(at -3 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V5" smd circle
		(at -2.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V6" smd circle
		(at -2 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V7" smd circle
		(at -1.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V8" smd circle
		(at -1 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "V9" smd circle
		(at -0.5 4)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W1" smd circle
		(at -4.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W10" smd circle
		(at 0 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W11" smd circle
		(at 0.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W12" smd circle
		(at 1 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W13" smd circle
		(at 1.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W14" smd circle
		(at 2 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W15" smd circle
		(at 2.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W16" smd circle
		(at 3 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W17" smd circle
		(at 3.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W18" smd circle
		(at 4 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W19" smd circle
		(at 4.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W2" smd circle
		(at -4 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W3" smd circle
		(at -3.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W4" smd circle
		(at -3 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W5" smd circle
		(at -2.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W6" smd circle
		(at -2 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W7" smd circle
		(at -1.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W8" smd circle
		(at -1 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "W9" smd circle
		(at -0.5 4.5)
		(size 0.275 0.275)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_BGA.3dshapes/Xilinx_CPG236.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
