(footprint "Analog_LFCSP-8-1EP_3x3mm_P0.5mm_EP1.53x1.85mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFCSP, exposed pad, Analog Devices (http://www.analog.com/media/en/technical-documentation/data-sheets/ADL5542.pdf)")
	(tags "LFCSP 8 0.5")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Analog_LFCSP-8-1EP_3x3mm_P0.5mm_EP1.53x1.85mm"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.37 -0.25)
		(size 0.71 0.28)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -1.37 0.25)
		(size 0.71 0.28)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.2 1.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.37 -0.25)
		(size 0.71 0.28)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.37 0.25)
		(size 0.71 0.28)
		(layers "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -1.37 -0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 -0.25)
		(size 3.45 0.28)
		(layers "F.Cu")
	)
	(pad "2" smd rect
		(at 0 0)
		(size 1.53 1.85)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 0 0.25)
		(size 3.45 0.28)
		(layers "F.Cu")
	)
	(pad "4" smd rect
		(at -1.37 0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.37 0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.37 -0.75)
		(size 0.71 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-8-1EP_3x3mm_P0.5mm_EP1.53x1.85mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
