(footprint "Dialog_WLCSP-34_4.54x1.66mm_Layout17x4_P0.25x0.34mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Dialog Semiconductor (Renesas) WLCSP-34, staggered array, 4.54x1.66mm, 34 Ball, 17x4 Layout, 0.25x0.34mm Pitch, https://www.renesas.com/us/en/document/dst/da7212-datasheet")
	(tags "CSP 34 0.25x0.34 34-ball")
	(property "Reference" "REF**"
		(at 0 -1.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "Dialog_WLCSP-34_4.54x1.66mm_Layout17x4_P0.25x0.34mm"
		(at 0 1.83 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A11" smd circle
		(at 0.5 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A13" smd circle
		(at 1 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A15" smd circle
		(at 1.5 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A17" smd circle
		(at 2 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -1.5 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at -1 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A7" smd circle
		(at -0.5 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A9" smd circle
		(at 0 -0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B10" smd circle
		(at 0.25 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B12" smd circle
		(at 0.75 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B14" smd circle
		(at 1.25 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B16" smd circle
		(at 1.75 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -1.75 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at -1.25 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at -0.75 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B8" smd circle
		(at -0.25 -0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -2 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C11" smd circle
		(at 0.5 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C13" smd circle
		(at 1 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C15" smd circle
		(at 1.5 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C17" smd circle
		(at 2 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -1.5 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at -1 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C7" smd circle
		(at -0.5 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C9" smd circle
		(at 0 0.17)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D10" smd circle
		(at 0.25 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D12" smd circle
		(at 0.75 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D14" smd circle
		(at 1.25 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D16" smd circle
		(at 1.75 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -1.75 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at -1.25 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at -0.75 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D8" smd circle
		(at -0.25 0.51)
		(size 0.2 0.2)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/Dialog_WLCSP-34_4.54x1.66mm_Layout17x4_P0.25x0.34mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
