(footprint "LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16-Lead Lead Frame Chip Scale Package, 3x3mm, 0.5mm pitch, 1.854mm thermal pad (CP-16-22, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/lfcspcp/cp_16_22.pdf)")
	(tags "LFCSP 16 0.5")
	(property "Reference" "REF**"
		(at 0 -2.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm"
		(at 0 2.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.45 -0.45)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.45 0.45)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.45 -0.45)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.45 0.45)
		(size 0.7 0.7)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.448 -0.75)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.448 -0.25)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.448 0.25)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.448 0.75)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.75 1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.25 1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.25 1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.75 1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.448 0.75)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.448 0.25)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.448 -0.25)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.448 -0.75)
		(size 0.813 0.305)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.75 -1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.25 -1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.25 -1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -0.75 -1.448)
		(size 0.305 0.813)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 1.854 1.854)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-16-1EP_3x3mm_P0.5mm_EP1.854x1.854mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
