(footprint "LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFCSP, 16 pin, 4x4mm, 2.1mm sq pad (http://www.analog.com/media/en/technical-documentation/data-sheets/ADG633.pdf)")
	(tags "LFCSP 16 0.65")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.525 -0.525)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.525 0.525)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.525 -0.525)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.525 0.525)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.8025 -0.975)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.8025 -0.325)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.8025 0.325)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.8025 0.975)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.975 1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.325 1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.325 1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.975 1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.8025 0.975)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.8025 0.325)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.8025 -0.325)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.8025 -0.975)
		(size 1.105 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.975 -1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.325 -1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.325 -1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -0.975 -1.8025)
		(size 0.35 1.105)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 2.1 2.1)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
