(footprint "LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFCSP, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/AD7682_7689.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
	(tags "LFCSP DFN_QFN")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.625 -0.625)
		(size 1.08 1.08)
		(layers "F.Paste")
		(roundrect_rratio 0.231481)
	)
	(pad "" smd roundrect
		(at -0.625 0.625)
		(size 1.08 1.08)
		(layers "F.Paste")
		(roundrect_rratio 0.231481)
	)
	(pad "" smd roundrect
		(at 0.625 -0.625)
		(size 1.08 1.08)
		(layers "F.Paste")
		(roundrect_rratio 0.231481)
	)
	(pad "" smd roundrect
		(at 0.625 0.625)
		(size 1.08 1.08)
		(layers "F.Paste")
		(roundrect_rratio 0.231481)
	)
	(pad "1" smd roundrect
		(at -1.9375 -1)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.9375 -0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.9375 0)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9375 0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.9375 1)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1 1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -0.5 1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0 1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.5 1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1 1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.9375 1)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.9375 0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.9375 0)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.9375 -0.5)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.9375 -1)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1 -1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 0.5 -1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0 -1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -0.5 -1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -1 -1.9375)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" thru_hole circle
		(at -1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" smd roundrect
		(at 0 0)
		(size 2.5 2.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "21" smd roundrect
		(at 0 0)
		(size 2.5 2.5)
		(layers "B.Cu")
		(roundrect_rratio 0.1)
	)
	(pad "21" thru_hole circle
		(at 0 1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
