(footprint "LFCSP-72-1EP_10x10mm_P0.5mm_EP5.3x5.3mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "LFCSP, 72 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1452_1451_1450.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "LFCSP NoLead")
	(property "Reference" "REF**"
		(at 0 -6.33 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFCSP-72-1EP_10x10mm_P0.5mm_EP5.3x5.3mm_ThermalVias"
		(at 0 6.33 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.566667 -1.566667)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at -1.566667 0)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at -1.566667 1.566667)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.566667)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at 0 0)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at 0 1.566667)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at 1.566667 -1.566667)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at 1.566667 0)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "" smd custom
		(at 1.566667 1.566667)
		(size 1.274978 1.274978)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.562812 -0.439083)
					(xy -0.439083 -0.562812)
					(xy 0.439083 -0.562812)
					(xy 0.562812 -0.439083)
					(xy 0.562812 0.439083)
					(xy 0.439083 0.562812)
					(xy -0.439083 0.562812)
					(xy -0.562812 0.439083)
				)
				(width 0.298709)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.9375 -4.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.9375 -3.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.9375 -3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.9375 -2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.9375 -2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.9375 -1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -4.9375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -4.9375 -0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -4.9375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -4.9375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -4.9375 0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -4.9375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -4.9375 1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -4.9375 2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -4.9375 2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -4.9375 3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -4.9375 3.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -4.9375 4.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -4.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -3.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -3.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -2.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -2.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -1.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -1.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -0.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 0.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 0.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 1.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 1.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 2.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 2.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 3.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 3.75 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 4.25 4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 4.9375 4.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 4.9375 3.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 4.9375 3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 4.9375 2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 4.9375 2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 4.9375 1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 4.9375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 4.9375 0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 4.9375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 4.9375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 4.9375 -0.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 4.9375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 4.9375 -1.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at 4.9375 -2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at 4.9375 -2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at 4.9375 -3.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at 4.9375 -3.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at 4.9375 -4.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at 4.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at 3.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at 3.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at 2.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at 2.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at 1.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at 1.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at 0.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at 0.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at -0.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at -0.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at -1.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at -1.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at -2.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at -2.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at -3.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at -3.75 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at -4.25 -4.9375)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "73" thru_hole circle
		(at -2.35 -2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -2.35 -0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -2.35 0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -2.35 2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -0.783333 -2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -0.783333 -0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -0.783333 0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at -0.783333 2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" smd rect
		(at 0 0)
		(size 5.3 5.3)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "73" smd rect
		(at 0 0)
		(size 5.3 5.3)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "73" thru_hole circle
		(at 0.783333 -2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 0.783333 -0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 0.783333 0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 0.783333 2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 2.35 -2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 2.35 -0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 2.35 0.783333)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 2.35 2.35)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-72-1EP_10x10mm_P0.5mm_EP5.3x5.3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
