(footprint "LFCSP-72-1EP_10x10mm_P0.5mm_EP6.15x6.15mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "72-Lead Frame Chip Scale Package - 10x10x0.9 mm Body [LFCSP]; (see https://www.intersil.com/content/dam/Intersil/documents/l72_/l72.10x10c.pdf)")
	(tags "LFCSP 0.5")
	(property "Reference" "REF**"
		(at 0 -6.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFCSP-72-1EP_10x10mm_P0.5mm_EP6.15x6.15mm"
		(at 0 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.4 -1.4)
		(size 2.5 2.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 1.4)
		(size 2.5 2.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 -1.4)
		(size 2.5 2.5)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 1.4)
		(size 2.5 2.5)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -4.9 -4.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.9 -3.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.9 -3.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.9 -2.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.9 -2.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.9 -1.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.9 -1.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.9 -0.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -4.9 -0.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -4.9 0.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -4.9 0.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -4.9 1.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -4.9 1.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -4.9 2.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -4.9 2.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -4.9 3.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -4.9 3.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -4.9 4.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -4.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -3.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -3.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -2.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -2.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -1.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -0.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -0.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 0.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 0.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 1.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 1.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 2.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 2.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.75 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 4.25 4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 4.9 4.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 4.9 3.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 4.9 3.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 4.9 2.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 4.9 2.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 4.9 1.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 4.9 1.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 4.9 0.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 4.9 0.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 4.9 -0.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 4.9 -0.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 4.9 -1.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 4.9 -1.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 4.9 -2.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 4.9 -2.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 4.9 -3.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 4.9 -3.75 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 4.9 -4.25 90)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 4.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 3.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 3.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 2.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 2.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 1.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 1.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at 0.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at 0.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -0.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -0.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -1.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -1.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at -2.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at -2.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at -3.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at -3.75 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at -4.25 -4.9)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 0 0)
		(size 6.15 6.15)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-72-1EP_10x10mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
