(footprint "LFCSP-VQ-48-1EP_7x7mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFCSP VQ, 48 pin, exposed pad, 7x7mm body (http://www.analog.com/media/en/technical-documentation/data-sheets/AD7951.pdf, http://www.analog.com/en/design-center/packaging-quality-symbols-footprints/symbols-and-footprints/AD7951.html)")
	(tags "LFCSP 48")
	(property "Reference" "REF**"
		(at 0 -4.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFCSP-VQ-48-1EP_7x7mm_P0.5mm"
		(at 0 4.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.08 -2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -2.08 -0.68)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -2.08 0.69)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -2.06 2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -0.68 -2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -0.68 -0.68)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -0.68 0.69)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -0.66 2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.69 -2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.69 -0.68)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.69 0.69)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.71 2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 2.07 -2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 2.07 -0.68)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 2.07 0.69)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 2.09 2.05)
		(size 1.1 1.1)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "1" smd rect
		(at -3.4 -2.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.4 -2.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.4 -1.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.4 -1.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.4 -0.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.4 -0.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.4 0.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.4 0.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.4 1.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.4 1.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.4 2.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.4 2.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -2.75 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -2.25 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.75 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -1.25 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -0.75 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -0.25 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 0.25 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.75 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.25 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.75 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.25 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 2.75 3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 3.4 2.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 3.4 2.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 3.4 1.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 3.4 1.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 3.4 0.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3.4 0.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.4 -0.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.4 -0.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 3.4 -1.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.4 -1.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.4 -2.25)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.4 -2.75)
		(size 0.81 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 2.75 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 2.25 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 1.75 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 1.25 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 0.75 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 0.25 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -0.25 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -0.75 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -1.25 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -1.75 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -2.25 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -2.75 -3.4)
		(size 0.3 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 0 0)
		(size 5.26 5.26)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-VQ-48-1EP_7x7mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
