(footprint "OnSemi_ODCSP36_BGA-36_6.13x6.13mm_Layout6x6_P1.0mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "OnSemi ODCSP36 (Case 570CP), 0.27mm pad, 6.13x6.13mm, 36 Ball, 6x6 Layout, 1.0mm Pitch, https://www.onsemi.com/pub/Collateral/570CP.PDF")
	(tags "CSP 36 1.0")
	(solder_mask_margin 0.1)
	(property "Reference" "REF**"
		(at 0 -4.065 0)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_ODCSP36_BGA-36_6.13x6.13mm_Layout6x6_P1.0mm"
		(at 0 4.065 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "+"
		(at 2.8 2.75 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2.5 -2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -1.5 -2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.5 -2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.5 -2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at 1.5 -2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 2.5 -2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -2.5 -1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -1.5 -1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.5 -1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.5 -1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at 1.5 -1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 2.5 -1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -2.5 -0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -1.5 -0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.5 -0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.5 -0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at 1.5 -0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 2.5 -0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -2.5 0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -1.5 0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.5 0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.5 0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at 1.5 0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at 2.5 0.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -2.5 1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -1.5 1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.5 1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0.5 1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E5" smd circle
		(at 1.5 1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E6" smd circle
		(at 2.5 1.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -2.5 2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -1.5 2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.5 2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0.5 2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F5" smd circle
		(at 1.5 2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at 2.5 2.5)
		(size 0.27 0.27)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/OnSemi_ODCSP36_BGA-36_6.13x6.13mm_Layout6x6_P1.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
