(footprint "ST_WLCSP-36_Die417"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "WLCSP-36, 2.61x2.88mm, 36 Ball, 6x6 Layout, 0.4mm Pitch, http://www.st.com/resource/en/datasheet/stm32l052t8.pdf#page=123")
	(tags "CSP 36 0.4")
	(solder_mask_margin 0.04)
	(solder_paste_margin 0.000001)
	(property "Reference" "REF**"
		(at 0 -2.44 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_WLCSP-36_Die417"
		(at 0 2.44 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1 -1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A2" smd circle
		(at -0.6 -1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A3" smd circle
		(at -0.2 -1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A4" smd circle
		(at 0.2 -1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A5" smd circle
		(at 0.6 -1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "A6" smd circle
		(at 1 -1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B1" smd circle
		(at -1 -0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B2" smd circle
		(at -0.6 -0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B3" smd circle
		(at -0.2 -0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B4" smd circle
		(at 0.2 -0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B5" smd circle
		(at 0.6 -0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "B6" smd circle
		(at 1 -0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C1" smd circle
		(at -1 -0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C2" smd circle
		(at -0.6 -0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C3" smd circle
		(at -0.2 -0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C4" smd circle
		(at 0.2 -0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C5" smd circle
		(at 0.6 -0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "C6" smd circle
		(at 1 -0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D1" smd circle
		(at -1 0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D2" smd circle
		(at -0.6 0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D3" smd circle
		(at -0.2 0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D4" smd circle
		(at 0.2 0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D5" smd circle
		(at 0.6 0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "D6" smd circle
		(at 1 0.2)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E1" smd circle
		(at -1 0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E2" smd circle
		(at -0.6 0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E3" smd circle
		(at -0.2 0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E4" smd circle
		(at 0.2 0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E5" smd circle
		(at 0.6 0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "E6" smd circle
		(at 1 0.6)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F1" smd circle
		(at -1 1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F2" smd circle
		(at -0.6 1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F3" smd circle
		(at -0.2 1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F4" smd circle
		(at 0.2 1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F5" smd circle
		(at 0.6 1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "F6" smd circle
		(at 1 1)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_CSP.3dshapes/ST_WLCSP-36_Die417.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
